For 1990-2009 cars

### Removal Procedure

1. Remove the rear window lower garnish molding. Refer to Rear Window Garnish Molding Replacement .
2. Remove the rear panel carpet retainers.
3. Remove the rear panel carpet (1).

### Installation Procedure

1. Install the rear panel carpet (1).
2. Install the carpet retainers.
3. Install the rear window lower garnish molding. Refer to Rear Window Garnish Molding Replacement .