For 1990-2009 cars

### Removal Procedure

1. Set the parking brake.
2. Block the front and the rear wheels.

Important: In order to maintain proper driveline alignment, some models may use spacers or shims between the torque rod and torque rod mounting bracket, or between the mounting bracket and the frame crossmember. Note the number and position of spacers or shims for proper installation.

3. Remove the following components from the torque mounting brackets and the axle bracket:

• | The nuts

• | The washers

• | The bolts

4. Remove the torque rod.

### Installation Procedure

Important: Use the same number of spacers or shims as previously used in order to ensure original driveline alignment.

1. Install the torque rod to frame mounting brackets.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the following components:

• | The torque rod bolt

• | The washers

• | The nuts

Tighten
Tighten the torque rod nut to 85 N·m (63 lb ft).

3. Install the torque rod to the axle mounting bracket.
4. Install the following components:

• | The torque rod bolts

• | The washers

• | The nuts

Tighten
Tighten the torque rod nut to 175 N·m (130 lb ft).