For 1990-2009 cars

## Battery Negative Cable Replacement Negative Cable to Frame

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable from the battery.
2. Disconnect the negative battery cable from the frame.
3. Disconnect the wires from the negative junction block.
4. Disconnect the negative junction from the frame.

### Installation Procedure

1. Connect the negative battery cable to the frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Clean the grounding area and coat the area with a copper-impregnated ground sealer.

Tighten
Tighten the cable to the frame bolt to 30 N·m (22 lb ft).

3. Connect the negative junction to the frame.
4. Connect the wires to the negative junction block.
5. Connect the negative battery cable to the battery.

## Battery Negative Cable Replacement Negative Cable to Engine

### Removal Procedure

1. Disconnect the negative cable from the starter.
2. Disconnect the negative cable from the frame.

### Installation Procedure

1. Connect the negative cable to the frame.

Clean the grounding area and coat it with a copper-impregnated ground sealer.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Connect the negative cable to the starter.

Tighten

• | Tighten the cable to the frame (7.2L) nut to 28 N·m (21 lb ft).

• | Tighten the cable to the starter (7.2L) nut to 30 N·m (22 lb ft).