For 1990-2009 cars

Important: Twist the spark plug boot 1/2 turn in order to release the boot. Pull on the spark plug boot only. Do not pull on the spark plug wire.

1. Remove the left spark plug wires from the spark plugs and ignition coils.
2. Remove the left exhaust manifold heat shield nuts.
3. Remove the left exhaust manifold heat shield.
4. Remove the left exhaust manifold nuts and center bolt.
5. Remove the left exhaust manifold.
6. Remove the left exhaust manifold gasket.
7. Remove the left spark plugs.
8. Remove the exhaust manifold studs, if necessary.