For 1990-2009 cars

#### Tools Required

• | J 43910 Output Shaft Bearing Puller Leg Set

• | J 24420-B Universal Puller

• | J 43769 Spanner Nut Wrench - 4WD

1. Position the transmission so that the rear of the transmission is facing up.
2. Remove the flange or yoke (1) from the output shaft (2).
3. If present, remove the oil seal assembly.

Important: The fullest clockwise position of the manual shift shaft is park (P), which engages the park pawl.

4. On 4WD transmissions only, use a wrench on the manual shift shaft flats to rotate the manual shift shaft to the fullest clockwise position.
5. On 4WD transmissions only, perform the following steps:

5.1. | Install J 43769 (1) onto the output nut (2).

5.2. | Remove the output nut (2).

6. Remove the retaining ring (1) from the low and reverse clutch housing (2).
7. Assemble the three legs of J 43910 to J 24420-B (2) .
8. Place the foot of each leg between the 2 bearing balls.
9. Twist each leg until the foot of the leg is forced under the bearing races.
10. Adjust the center screw (4) and each leg nut (1) until the body of J 24420-B is perpendicular to the rear face of the transmission case.
11. Tighten the center screw (4) until ball bearing assembly (3) is dislodged.
12. Remove J 43910 ,J 24420-B , and J 43769 from the ball bearing assembly.
13. For both transmissions, remove the selective spacer (1).