For 1990-2009 cars

## Engine Flywheel Housing Installation Automatic Transmission

1. Install the transmission converter covers.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission converter cover bolts.

Tighten
Tighten the transmission converter cover bolts to 12 N·m (106 lb in).

3. Install the engine flywheel housing.
4. Install the engine flywheel housing bolts.

Tighten
Tighten the flywheel housing bolts to 67 N·m (49 lb ft).

## Engine Flywheel Housing Installation Manual Transmission

1. Install the engine flywheel housing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine flywheel housing bolts.

Tighten
Tighten the engine flywheel housing bolts to 60 N·m (44 lb ft).