For 1990-2009 cars

### Removal Procedure

Notice: Do not start the vehicle with any power steering gear inlet or outlet hoses disconnected. When disconnected, plug or cap all openings of components. Failure to do so could result in contamination or loss of power steering fluid and damage to the system.

1. Siphon the power steering fluid from the reservoir.
2. Disconnect the hose from the pump.
3. Disconnect the hose from the reservoir.
4. Remove the hose from the vehicle.

### Installation Procedure

1. Install the hose to the power steering pump.
2. Install the hose to the power steering reservoir.

Make sure the clamp is positioned at the end of the hose.

3. Fill the power steering reservoir with fluid. Refer to Checking and Adding Power Steering Fluid .
4. Bleed the power steering system. Refer to Power Steering System Bleeding .