For 1990-2009 cars

### Removal Procedure

1. Block the wheels.
2. Release the parking brake.
3. Remove the jam nut on the actuator end of the cable at the 2-piece fitting.
4. Remove the end fitting.
5. Remove the cotter pin.
6. Remove the cable clevis pin.
7. Remove the fastener from the transmission bracket clip.
8. Remove the fastener from the transmission housing bracket.
9. Remove the fastener from the frame bracket.
10. Remove the strap.
11. Remove the cable assembly.

### Installation Procedure

1. Install the new cable assembly.
2. Install the strap.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fastener to the frame bracket.

Tighten
Tighten the fastener bracket to 50 N·m (37 lb ft).

4. Install the fastener to the transmission housing bracket.

Tighten
Tighten the fastener bracket to 35 N·m (26 lb ft).

Notice: Make sure that the clip has the bolt hole facing forward. If the clip is out of position, it may cause a binding condition in the parking brake released position.

5. Install the fastener from the transmission bracket clip.

Tighten
Tighten the fastener 64 N·m (47 lb ft).

6. Install the small and the large ends of the two-piece cable fitting at the actuator.
7. Ensure that the small fitting bottoms at both the actuator and the large half of the two-piece fitting.

Tighten
Torque the two pieces of the fitting together to 54 N·m (40 lb ft).

8. Install the jam nut to the 2-piece fitting.

Tighten
Tighten the jam nut to 45 N·m (33 lb ft).

9. Adjust the park brake lever. Refer to Park Brake Adjustment .
10. Remove the wheel blocks.