For 1990-2009 cars

## Power Steering Fluid Reservoir Replacement Radiator Suport Mounted

### Removal Procedure

1. Drain the reservoir.

Important: Cap the hoses in order to prevent dirt from entering the system.

2. Remove the hoses (2, 3) from the reservoir (1).
3. Remove the following components:

3.1. | The bolts (7) and washers (8)

3.2. | The reservoir (1)

### Installation Procedure

1. Install the reservoir (1) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the washers (8) and the bolts (7).

Tighten
Tighten the reservoir mounting bolts to 28 N·m (21 lb ft).

3. Connect the hoses (2, 3) to the reservoir (1).
4. Bleed the system. Refer to Power Steering System Bleeding .