For 1990-2009 cars

### Removal Procedure

1. Open hood.
2. If equipped, unclip engine harness and position to gain access to the front of the air cleaner housing.
3. Release the air cleaner housing top clips.
4. Open the air cleaner top and pull the air cleaner top toward the front of the vehicle to disengage the air cleaner top retain fingers and remove air cleaner top from cleaner bottom.
5. Remove air cleaner element from air cleaner bottom.
6. If equipped, remove the inner filter element from the air cleaner element.

### Installation Procedure

1. Wipe the air cleaner bottom clean of all debris.
2. If equipped, install the inner filter element into the filter element.
3. Install the air cleaner element in the air cleaner bottom.
4. Position the air cleaner top retainer fingers into the air cleaner bottom.
5. Engage the air cleaner clips.
6. If equipped, reposition the engine harness and install retainers.