For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Crankshaft Position Variation Learn | -- | Enables the powertrain control module (PCM) to learn the variations in the crankshaft position (CKP) system. The PCM will learn the variations once the following conditions are met:

• | Engine coolant temperature (ECT) is more than a specified value.

• | All instructions on the scan tool have been completed.

• | The accelerator pedal is smoothly applied until the fuel cut-OFF, as specified on the scan tool, is achieved, and then immediately released.

The PCM learns the variation values on the deceleration from fuel cut-OFF.

Cylinder Power Balance | Fuel System | Enables/Disables a cylinder by turning OFF the fuel injector to the cylinder. The fuel injector is normally enabled. The PCM disables the fuel injector when the following conditions are met:

• | All instruction on the scan tool are completed

• | Stabilized engine speed

• | The fuel injector is selected

When the Disable is selected the PCM turns the injector OFF for 30 seconds. During this period, the engine operates with a misfire.

Engine Speed Control | TAC System | Activates the throttle activation control (TAC) system to change engine RPM. The normal commanded state is None. To enable the RPM control, all instruction on the scan tool must be completed. The system will increase or decrease the RPM within a range of 350-2,000 RPM. The set step value changes the RPM by increments of 25 RPM, 100 RPM, and 500 RPM. The system remains in the commanded state until cancelled by the scan tool.
EVAP Purge Solenoid | Engine Output Controls/EVAP System | Activates the evaporative emission (EVAP) purge valve. The normal commanded state is None. The system will increase or decrease the amount of EVAP purge valve opening by 10 percent increments within a range of 0-100 percent. The system remains in the commanded state until cancelled by the tool or the fuel tank pressure (FTP) exceeds 32 mm Hg (17 in H20).
EVAP System Seal | Engine Output Controls/EVAP System | Commands the purge valve OFF, closed, and the vent valve ON (closed). The system will remain in the commanded state until commanded off with the scan tool.
EVAP Test | Service Bay Test | Activates the Service Bay Test to verify the integrity of the EVAP system. The scan tool initiates the test when the following conditions are met:

• | All instruction on the scan tool have been completed

• | ECT is less than a specified value

• | No DTCs are set

Fuel Injector Balance | Fuel System | Enables the fuel injector in order to verify proper fuel injector flow. The PCM will pulse the selected injector when the following conditions are met:

• | All instruction on the scan tool completed

• | Fuel injector selected

• | Key ON, engine OFF

The selected fuel injector can only be flowed/pulsed once per ignition cycle.

Fuel Pump | Engine Output Controls | Controls the fuel pump relay. The normal commanded state is None. When commanded ON/OFF, the PCM turns the fuel pump ON/OFF. If the engine is running, and the fuel pump is commanded OFF, the engine will stall. The system remains in the commanded state until cancelled by the scan tool.
Fuel Trim Enable | Fuel System | Disables the PCMs ability to learn new fuel trim parameters. The system remains in the commanded state until cancelled by the scan tool.
Fuel Trim Reset | Fuel System | Activates the reset of fuel trim data in all of the fuel trim cells.
Loop Status | Engine Output Controls | Controls the system loop status. The commanded states include None, Open, or Closed. The normal commanded state is None. When commanded Open or Closed, the system remains in the commanded state until cancelled by the scan tool.
Malfunction Indicator Lamp | Engine Output Controls | Controls the malfunction indicator lamp (MIL). The commanded states include None, ON, and OFF. When commanded ON or OFF, the system remains in the commanded state until cancelled by the scan tool.
Misfire Graph | -- | Graphs the accumulated misfires occurring in each cylinder. The scan tool allows for a reset of the misfire graph.
O2S Heater Control | Engine Output Controls | Activates the HO2S Heater. The commanded states include None, ON, and OFF. The normal commanded state is None. On a cold engine, with the key ON, engine OFF, the HO2S signal will continue to drop below bias when commanded ON. The system remains in the commanded state until cancelled by the tool.