For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the door trim panel. Refer to Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Door Water Deflector Replacement .
4. Remove the inner mounting panel. Refer to Door Mounting Panel Replacement - Inner .
5. Remove the lock actuator mounting rivets by drilling.
6. Remove the remote lock rod (2) from the actuator arm.
7. Remove the wiring harness from the lock actuator.
8. Remove the actuator from the module panel.

### Installation Procedure

1. Install the inner mounting panel to actuator rivets.
2. Install the wiring harness to the actuator.
3. Install the remote lock rod (2) to the actuator arm.
4. Install the module panel to the door.
5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Door Trim Panel Replacement
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.