For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Block the wheels.
3. Remove the retaining bolts and bracket.
4. Disconnect the electrical connector.
5. Remove the park control module.

### Installation Procedure

1. Install the park control module.
2. Connect the electrical connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the bracket and retaining bolts.

Tighten
Tighten the retaining bolts to bracket 2.5 N·m (22 lb in).

4. Remove the wheel blocks.