For 1990-2009 cars

### Removal Procedure

1. Disconnect the wiring harness from the hourmeter.
2. Remove the 2 nuts from the back of the hourmeter.
3. Remove the screws.
4. Move the hourmeter rearward in order to remove the hourmeter from the bracket.

### Installation Procedure

1. Install the hourmeter to the bracket
2. Install the screws.
3. Install the 2 nuts to the back of the hourmeter.
4. Connect the wiring harness to the hourmeter.