For 1990-2009 cars

### Removal Procedure

1. Roll the window up.
2. Remove the trim panel. Refer to Door Trim Panel Replacement .
3. Remove the door to window channel bolt.
4. Remove the run channel from the door.

### Installation Procedure

1. Install the window channel to the door.
2. Place the lip of the lower channel into the upper channel.
3. Install the door to window channel bolt.
4. Install the trim panel. Refer to Door Trim Panel Replacement .