For 1990-2009 cars

### Removal Procedure

1. Remove the door sill trim plate. Refer to Door Sill Plate Replacement .
2. Remove the hinge pillar trim panel screw (2).
3. Remove the hinge pillar trim panel (1).

### Installation Procedure

1. Install the hinge pillar trim panel (1).
2. Install the hinge pillar trim panel screw (2).
3. Install the door sill trim plate. Refer to Door Sill Plate Replacement .