For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Dryer Delivery Port Elbow* | 35 N·m | 26 lb ft
Air Dryer Governor Port Elbow* | 20 N·m | 15 lb ft
Air Dryer Nut | 45 N·m | 33 lb ft
Air Dryer Support Elbow* | 35 N·m | 26 lb ft
Air Reservoir Plug | 50 N·m | 37 lb ft
Air Reservoir Support Bolt (All except Rear Axle Rear Unit without Reinforced Frame) | 53 N·m | 39 lb ft
Air Reservoir Support Bolt (Rear Axle Rear Unit without Reinforced Frame) | 45 N·m | 33 lb ft
Bracket Bolt | 12 N·m | 106 lb in
Brake Pedal Bracket Bolt (6 mm) | 8 N·m | 71 lb in
Brake Pedal Bracket Bolt (8 mm) | 19 N·m | 14 lb ft
Brake Pedal Joint Lock Nut | 62 N·m | 46 lb ft
Double Check Valve | 28 N·m | 21 lb ft
Dual Application Valve Mounting Bolt | 40 N·m | 29 lb ft
Elbow* (Trailer Air Brake Service and Emergency Coupling Bracket Connectors) | 28 N·m | 21 lb ft
Elbow* (Truck Trailer Air Brake Coupling Stud Nut) | 20 N·m | 15 lb ft
Front Axle Service Reservoir Support Bolts | 67 N·m | 49 lb ft
Front Axle Limiting, Ratio Valve Nuts | 22 N·m | 16 lb ft
Inflation Valve | 20 N·m | 15 lb ft
Low Air Pressure Switch | 12 N·m | 106 lb in
Male Connector (Trailer Air Brake Service and Emergency Coupling Bracket) | 28 N·m | 21 lb ft
Male Connector Nut (Trailer Air Brake Service and Emergency Coupling Bracket) | 12 N·m | 106 lb in
Park Control Valve Nut (Cab Mounted) | 6 N·m | 53 lb in
Park Control Valve Nut (Chassis Mounted) | 22 N·m | 16 lb ft
Parking Control Valve Nut | 6 N·m | 53 lb in
Pogo Stick Nut | 28 N·m | 21 lb ft
Pressure Protection Valve Nut | 30 N·m | 22 lb ft
Quick Release Valve (Double Check Type) Bolt | 52 N·m | 38 lb ft
Quick Release Valve Nut | 22 N·m | 16 lb ft
Rear axle service, truck, nuts | 42 N·m | 31 lb ft
Relay Valve Bolt | 52 N·m | 38 lb ft
Relay Valve (Double Check Type) Bolt | 52 N·m | 38 lb ft
Relay Valve (Proportioning Type) Bolt | 52 N·m | 38 lb ft
Reservoir Drain Valve | 50 N·m | 37 lb ft
Reservoir Drain Valve (Manual Type) | 50 N·m | 37 lb ft
Safety Valve | 30 N·m | 22 lb ft
Single Check Valve | 50 N·m | 37 lb ft
Stoplamp Switch | 11 N·m | 97 lb in
Strap Nut (All except Rear Axle Front Unit and Repair Axle Rear Unit Air Reservoirs) | 28 N·m | 21 lb ft
Strap Nut (Rear Axle Front Unit and Repair Axle Rear Unit Air Reservoirs) | 23 N·m | 17 lb ft
Stud Nut (Truck Trailer Air Brake Coupling) | 45 N·m | 33 lb ft
Stop Lamp Switch | 12 N·m | 106 lb in
Towing Vehicle Protection Valve Nut | 22 N·m | 16 lb ft
Trailer Air Brake Control Valve Bolt | 40 N·m | 29 lb ft
Trailer Air Brake Coupling (Truck) | 35 N·m | 26 lb ft
Trailer Air Brake Dummy Coupling Nut (Truck) | 30 N·m | 22 lb ft
Trailer Air Brake Emergency Coupling Hose (Tractor) | 28 N·m | 21 lb ft
Trailer Air Brake Service Coupling Hose (Tractor) | 28 N·m | 21 lb ft
Trailer Air Brake Stoplamp Switch | 7 N·m | 62 lb in
*Tighten to the specified torque, and then rotate a maximum of 360 degrees until the proper orientation is achieved.