For 1990-2009 cars

## Roof Marker Lamp Replacement Delete

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the lens screws.
3. Remove the lens.
4. In order to remove the insulator, pull the socket and harness assembly through the insulator.
5. Disconnect the harness assembly electrical connector.

### Installation Procedure

1. Connect the harness assembly electrical connector.
2. In order to install the insulator, push the socket and harness assembly into the insulator and align the holes on the cab.
3. Install the lens.
4. Install the lens screws.
5. Connect the negative battery cable.