For 1990-2009 cars

## Evaporative Emission Hoses/Pipes Replacement - Canister/Fuel Tank C4500 and C5500

Caution: Refer to Fuel Vapors in Evaporative Emission Components Caution in the Preface section.

Caution: Refer to Fuel and Evaporative Emission Pipe Caution in the Preface section.

### Removal Procedure

1. Disconnect the evaporative emission (EVAP) vapor pipe from the EVAP canister.
2. Remove the fuel tank. Refer to Fuel Tank Replacement .
3. Disconnect the EVAP vapor pipe from the fuel sender assembly.
4. Remove the EVAP vapor pipe.

### Installation Procedure

1. Install the EVAP vapor pipe to the fuel sender assembly.
2. Install the fuel tank. Refer to Fuel Tank Replacement .
3. Connect the fuel tank EVAP vapor pipe to the EVAP canister.