For 1990-2009 cars

1. Remove the camshaft retainer bolts.
2. Remove the camshaft retainer.
3. Install three 8-1.25 x 100 mm bolts in the camshaft front bolt holes.

Notice: All camshaft journals are the same diameter, so care must be used in removing or installing the camshaft to avoid damage to the camshaft bearings.

4. Using the bolts as a handle, carefully rotate and pull the camshaft out of the engine block.
5. Remove the bolts from the front of the camshaft.