For 1990-2009 cars

Important:

• | Measure as described below at a minimum of 3 locations.

• | Replace any 4-5 clutch fiber plate that does not meet specifications.

1. Measure the thickness of each 4-5 clutch fiber plate (1) at dimension A.

Specification
The 4-5 clutch fiber plate minimum thickness is 2.375 mm (0.0935 in).

2. Measure the 4-5 clutch fiber plate oil groove depth of each plate at dimension B.

Specification
The 4-5 clutch fiber plate minimum groove depth is 0.200 mm (0.0079 in).