For 1990-2009 cars

### Removal Procedure

1. Disconnect the clutch pedal position switch electrical connector.
2. Slide the switch to the right in order to disengage the switch from the bracket.
3. Remove the clutch pedal position switch.

### Installation Procedure

1. Install the clutch pedal position switch.
2. Slide the switch to the left in order to engage the switch to the bracket.
3. Connect the clutch pedal position switch electrical connector.