For 1990-2009 cars

## Body Side Outside Assist Handle Replacement NWR

### Removal Procedure

1. Remove the following parts from the handle and heat shield:

• | The bolts

• | The washers

• | The nuts

2. Remove the handle from the vehicle.

### Installation Procedure

1. Place the handle in the correct position on the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the handle and heat shield with the following components:

• | The bolts

• | The washers

• | The nuts

Tighten
Tighten the handle bolts to 11 N·m (8 lb in).

## Body Side Outside Assist Handle Replacement NB5

### Removal Procedure

1. Remove the 2 bolts from the handle.
2. Remove the handle from the vehicle.

### Installation Procedure

1. Place the handle in the correct position on the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the handle.

Install the 2 bolts.

Tighten
Tighten the handle bolts to 11 N·m (8 lb in).