For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle with safety stands. Refer to Lifting and Jacking the Vehicle .
2. Remove the engine front mount bracket to engine front mount bolt.
3. Lift the engine to take the weight off the mounts.
4. Remove the engine mount bracket to engine bolt.
5. Remove the engine mount bracket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine mount bracket to the engine.
2. Install the engine mount bracket to engine bolts.

Tighten
Tighten the engine mount bracket to engine bolts to 130 N·m (96 lb ft).

3. Lower the engine on to the front engine mounts.
4. Install the engine front mount brackets to engine front mount bolt .

Tighten
Tighten the engine front mount bolts to 240 N·m (178 lb ft).

5. Remove the safety stands.
6. Lower the vehicle.