For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .
2. Remove the belt tensioner bolt.
3. Remove the belt tensioner.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the drive belt tensioner.
2. Install the drive belt tensioner bolt.

Tighten
Tighten the drive belt tensioner bolt to 50 N·m (37 lb ft).

3. Install the drive belt. Refer to Drive Belt Replacement .