For 1990-2009 cars

#### Tools Required

• | J 43320 Crankshaft Rear Seal Puller

• | J 42849 Crankshaft Rear Seal Installer

### Removal Procedure

1. Remove the flywheel. Refer to Engine Flywheel Replacement .
2. Install the guide pins from J 43320 into the crankshaft.
3. Install the J 43320 over the guide pins.
4. Using a suitable drill, insert eight of the self-tapping sheet metal screws into the rear crankshaft seal, using a criss-cross pattern. The self-tapping screws are included with the J 43320 .
5. Thread the center bolt of J 43320 into the crankshaft to remove the seal.
6. Remove the guide pins from the crankshaft.

### Installation Procedure

1. Make sure the crankshaft rear chamfer is free of grit, loose rust, and burrs. Correct as needed.
2. Apply a very light film of oil onto the crankshaft sealing surface. DO NOT apply oil to the sealing surface of the engine block.
3. Install the seal onto J 42849 .
4. Position the J 42849 against the crankshaft. Thread the attaching screws into the tapped holes in the crankshaft.
5. Tighten the screws securely with a screwdriver in order to insure that the seal is installed squarely over the crankshaft.
6. Rotate the center nut until the J 42849 bottoms.
7. Remove the J 42849 .
8. Install the flywheel. Refer to Engine Flywheel Replacement .