For 1990-2009 cars

#### Tools Required

• | J 43791 Output/Turbine Shaft Bushing Installer

• | J 44526 Output/Turbine Shaft Bushing Remover

### Removal Procedure

1. Install J 44526-2 bolt (8) and J 44526-1 extractor (7) into the bushing (9) .
2. Install J 44526-2 bolt (8) into J 44526-1 extractor (7) .
3. Install the washer (6) and nut (5) onto J 44526-2 bolt (8).
4. Hold the top of J 44526-2 bolt (8) with a wrench and tighten the nut (5) until J 44526-1 extractor (7) engages the bushing (9) .
5. Install the bearing (3), washer (2), and nut (1) onto J 44526-2 bolt (8) .
6. Install J 44526-3 protector (4) onto J 44526-2 bolt (8) .
7. Hold the top of J 44526-2 bolt (8) with a wrench and tighten the nut (1) until the bushing is dislodged .
8. Remove the J tools.
9. Remove the bushing from J 44526 .

### Installation Procedure

1. Install a new output shaft bushing (2) onto J 43791 (1).
2. Using J 43791 , drive the bushing into the output shaft (3) until J 43791 (1) is seated to specification.

Specification
Make sure the bushing is pressed flush to 0.25 mm (0.01 in) below the output shaft surface.