For 1990-2009 cars

## Parking Brake Lever Replacement Mechanical

### Removal Procedure

1. Remove the clevis pin from the cable and lever assembly.
2. Remove the mounting bolts.
3. Remove the park brake warning lamp switch bolt.
4. Remove the park brake warning lamp switch.
5. Disconnect the electrical connector.
6. Remove the cable from the lever.
7. Remove the parking brake lever.

### Installation Procedure

1. Connect the electrical connector.
2. Install the park brake warning lamp switch.
3. Install the park brake warning lamp switch bolt.
4. Install the cable to the park brake lever.
5. Install the park brake lever assembly.
6. Install the mounting bolts.
7. Adjust the parking brake

## Parking Brake Lever Replacement Electric/Hydraulic

### Removal Procedure

1. Remove the console assembly.
2. Remove the mounting bolts.
3. Remove the parking brake lever.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the parking brake lever to the cab.
3. Install the mounting bolts.
4. Install the console assembly.