For 1990-2009 cars

#### Tools Required

• | J 43785 Intermediate Bushing Remover/Installer

• | J 8092 Universal Driver

Important: The preferred method for removing/installing the intermediate carrier bushing is to use J 43785 and a press. If a press is not available, use J 43785 and universal driver J 8092 .

1. Position the intermediate carrier assembly (3) on wooden blocks on the press with the external splines facing up.
2. If the bushing will be removed with out a press, install the short end of J 43785 (2) ontoJ 8092 (1).
3. Using J 43785 (2), press or drive the bushing (4) out of the carrier (3).
4. Position the intermediate carrier assembly (4) on wooden blocks on the press with the external splines facing down.
5. If the bushing will be installed without a press, install the long end of J 43785 (2) ontoJ 8092 (1).
6. Install a new bushing (3) onto J 43785 (2).
7. Using J 43785 (2), press or drive the bushing into of the carrier until J 43785 (2) seats.