For 1990-2009 cars

### Removal Procedure

1. Unscrew the knob from the hazard warning switch.
2. Remove the nut from the hazard warning switch.
3. Push the hazard warning switch through the hole.
4. Disconnect the electrical connector from the hazard warning switch.
5. Pull the HAZARD name plate from the instrument panel.
6. Disconnect the electrical connector from the HAZARD name plate.

### Installation Procedure

1. Connect the electrical connector to the HAZARD name plate.
2. Install the HAZARD name plate into the instrument panel.
3. Connect the electrical connector to the hazard warning switch.
4. Install the hazard warning switch through the hole in the instrument panel.
5. Install the nut to the hazard warning switch.
6. Screw the knob to the hazard warning switch.