For 1990-2009 cars

#### Tools Required

• | J 43781 Input Carrier Bushing Remover/Installer

• | J 8092 Universal Driver

Important: The preferred method for removing/installing the input carrier bushing is to use J 43781 and a press. If a press is not available, use J 43781 and J 8092 universal driver.

1. Position the input carrier assembly (3) on the press with the external splines facing up.
2. If the bushing will be removed without a press, install the short end of J 43781 (2) ontoJ 8092 (1).
3. Using J 43781 , press or drive the bushing (4) out of the carrier.
4. If the bushing will be installed without a press, install the long end of J 43781 (2) onto J 8092 (1).
5. Install a new bushing (3) onto J 43781 (2).
6. Using J 43781 , press or drive the bushing into the carrier until J 43781 (2) seats.