For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Terminal Nuts | 23 N·m | 17 lb ft
Battery Hold Down Retainer Nuts | 17 N·m | 13 lb ft
Fan Pulley Bolts (L18) | 45 N·m | 33 lb ft
Generator Adjusting Bracket Mounting Bolts (LG5) | 73 N·m | 54 lb ft
Generator Brace Bolts | 50 N·m | 37 lb ft
Generator Bracket Bolts and Nut (L18) | 41 N·m | 30 lb ft
Generator Mounting Bolts (L18) | 50 N·m | 37 lb ft
Generator Mounting Bottom Bolts (LG5) | 71 N·m | 52 lb ft
Generator Mounting Top Bolts (LG5) | 88 N·m | 65 lb ft
Generator Output Terminal Nut | 8 N·m | 71 lb in
Generator Shaft Nut | 100 N·m | 75 lb ft
Ground Strap to Engine Bolt (LG5) | 32 N·m | 24 lb ft
Ground Strap to Engine Bolt (L18) | 17 N·m | 13 lb ft
Ground Strap to Generator Bolt (LG5) | 11 N·m | 97 lb in
Ground Strap to Generator Bolt (L18) | 45 N·m | 33 lb ft
Negative Cable to Frame Bolt | 30 N·m | 22 lb ft
Negative Cable to Starter Bolt | 28 N·m | 21 lb tf
Positive Cable to Engine Bolt | 30 N·m | 22 lb ft
Positive Cable to Frame Bolt | 30 N·m | 22 lb ft
Positive Cable to Starter Nut | 30 N·m | 22 lb ft
Positive Cable to Starter Solenoid Nut (LG5) | 3 N·m | 27 lb in
Positive Cable to Starter Solenoid Nut (L18) | 10 N·m | 89 lb in
Starter Motor Bolt (LG5) | 70 N·m | 52 lb ft
Starter Motor Bolt--Automatic Transmission (L18) | 50 N·m | 37 lb ft
Starter Motor Bolt--Manual Transmission (L18) | 67 N·m | 49 lb ft
Wiring Harness Lead Nut to Generator Stud | 8 N·m | 71 lb in
Wiring Harness to Generator Bracket Bolt (L18) | 24 N·m | 18 lb ft