For 1990-2009 cars

## Transmission Range Select Control Valve Air Supply Tube Replacement Crossmember Mounted

### Removal Procedure

1. Bleed all air pressure from the system.
2. Remove the air supply tube from the elbow.
3. Remove the air supply tube from the pressure regulator valve.
4. Remove either 2 or 6 straps securing the supply tube.

### Installation Procedure

Important: Inspect the air supply tube fittings for damage prior to installation.

1. Install the air supply tube to the elbow.
2. Install the air supply tube to the pressure regulator valve.
3. Install either 2 or 6 straps securing the supply tube.

## Transmission Range Select Control Valve Air Supply Tube Replacement Frame Mounted

### Removal Procedure

1. Bleed all air pressure from the system.
2. Remove the air supply tube from the elbow.
3. Remove the air supply tube from the pressure regulator valve.
4. Remove the 4 straps securing the air supply tube.

### Installation Procedure

Important: Inspect the air supply tube fittings for damage prior to installation.

1. Install the air supply tube to the elbow.
2. Install the air supply tube to the pressure regulator valve.
3. Install the 4 straps securing the air supply tube.