For 1990-2009 cars

Condition | Action
--- | ---
Caution: While engine is operating, the exhaust system will become extremely hot. To prevent burns avoid contacting a hot exhaust system. DEFINITION: An audible or physical noise due to a faulty component or damaged components causing a loose or misaligned exhaust system resulting in a rattle or vibration noise (buzz, groan, hum).
Popping or hissing noise | Exhaust leak. Refer to Exhaust Leakage .
Loud exhaust |

1. Compare to a known good vehicle.
2. Inspect for a damaged or failed muffler.
3. Replace the faulty muffler. Refer to Muffler Replacement .

External rattle or vibration noise |

1. Inspect for a bent or loose hanger, loose heat shield, or loose clamp.
2. Inspect for a exhaust pipe causing interference.
3. Repair or replace the affected component.
4. Refer to the affected component service procedure.

Internal rattle |

1. Test the components by tapping with a rubber mallet to confirm a rattle.
2. Replace the faulty catalytic converter or muffler. Refer to the following procedures:

• | Catalytic Converter Replacement

• | Muffler Replacement