For 1990-2009 cars

Important: The oil pump pipe has a press fit into the oil pump. DO NOT remove the pipe from the oil pump. The pipe and oil pump are serviced as a complete assembly.

1. Remove the oil pump driveshaft and retainer.
2. Remove the oil pump cover bolts.
3. Remove the pump cover.
4. Remove the drive gear and the driven gear. Matchmark the gear teeth for assembly.
5. Remove the following items:

5.1. | The retaining pin

5.2. | The pressure relief valve spring

5.3. | The pressure relief valve