For 1990-2009 cars

### Removal Procedure

1. Set the parking brake.
2. Block the vehicle's rear wheels.
3. Remove the following components connecting the stabilizer link to the stabilizer bar:

• | The nut (11)

• | The washers (9)

• | The bolt (8)

4. Remove the following components connecting the stabilizer link to the frame bracket:

• | The nut (12)

• | The washers (17)

• | The bolt (18)

5. Remove the stabilizer links (10).

### Installation Procedure

1. Position the stabilizer links (10) to the vehicle.
2. Align the stabilizer link holes with the frame bracket and the stabilizer bar.

Important: Install the link mounting bolts from the outside of the link.

3. Install the following components:

• | The bolts (8, 18)

• | The washers (9, 17)

• | The nuts (11, 12)

Tighten
Tighten the stabilizer link nuts (11, 12) to 240 N·m (177 lb ft).

4. Remove the blocks from the wheels.