For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Pedal Bracket Mounting Nuts | 36 N·m | 27 lb ft
Air Cleaner Bracket Bolts | 25 N·m | 18 lb in
Air Cleaner Assembly Bolts | 5 N·m | 4 lb ft
Air Cleaner Inlet Clamp | 2.5 N·m | 22 lb in
Camshaft Position (CMP) Sensor Bolt | 12 N·m | 106 lb in
Crankshaft Position (CKP) Sensor Bolt | 12 N·m | 106 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Bracket Nut | 5 N·m | 44 lb in
Evaporative Emission (EVAP) Canister to Step Nut | 25 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Purge Valve Shoulder Bolt | 10 N·m | 89 lb in
Evaporative Emission (EVAP) Canister Retaining Bolt | 22.5 N·m | 17 lb ft
Fuel Fill Hose Clamp | 2.5 N·m | 22 lb in
Fuel Fill Pipe Ground Strap Bolt | 9 N·m | 80 lb in
Fuel Fill Pipe Housing to Fill Pipe Bolts | 2.3 N·m | 20 lb in
Fuel Filter Fitting | 27 N·m | 20 lb ft
Fuel Rail Attaching Bolts | 12 N·m | 106 lb in
Fuel Tank (Rear) Strap Bolts | 35 N·m | 26 lb ft
Fuel Tank (Mid Mount) Strap Bolts C 4 / 5 | 40 N·m | 30 lb ft
Fuel Tank Strap Nuts C 6 / 7 / 8 | 175 N·m | 129 lb ft
Fuel Tank (Rear) Attaching Bolts | 85 N·m | 63 lb ft
Fuel Tank (Rear) Shield Bolts | 175 N·m | 129 lb ft
Fuel Tank (15 gal) Shield Bolts | 85 N·m | 63 lb ft
Fuel Tank (15 gal) Shield Nuts | 85 N·m | 63 lb ft
Heated Oxygen Sensor (HO2S) | 41 N·m | 30 lb ft
Ignition Coil Attaching Bolts | 12 N·m | 106 lb in
Knock Sensor (KS) | 19 N·m | 14 lb ft
MAP Sensor Retaining Bolt | 12 N·m | 106 lb in
Maxi Fuse Block Bolt | 9 N·m | 80 lb in
Multi-Use Module Bracket Nuts | 25 N·m | 18 lb in
Powertrain Control Module (PCM) Connector End Bolts | 8 N·m | 70 lb in
Throttle Actuator Control (TAC) Module Nuts | 9 N·m | 80 lb in
Throttle Body Attaching Nuts | 10 N·m | 89 lb in