For 1990-2009 cars

Important: Twist the spark plug boot 1/2 turn in order to release the boot. Pull on the spark plug boot only. Do not pull on the spark plug wire.

1. Remove the right spark plug wires from the spark plugs and ignition coils.
2. Remove the right exhaust manifold heat shield nuts.
3. Remove the right exhaust manifold heat shield.
4. Remove the right exhaust manifold nuts and center bolt.
5. Remove the right exhaust manifold.
6. Remove the right exhaust manifold gasket.
7. Remove the right spark plugs.
8. Remove the exhaust manifold studs, if necessary.