For 1990-2009 cars

Important: Perform the following steps in sequence BEFORE proceeding to the engine vibration analysis tables.

1. Perform the Vibration Analysis - Road Testing table in order to duplicate and effectively diagnose the customer's concern.
2. If powertrain related DTCs are present, there may be a powertrain performance condition present which could be a contributing cause to the customer's concern. Using a scan tool, determine if any DTCs are set. If DTCs have been set, refer to Diagnostic System Check - Engine Controls in Engine Controls - 8.1L.
3. After the Vibration Analysis -- Road Testing is complete and there are no DTCs which affect the customer's concern, go to Vibration Analysis - Engine/Accessory Isolation .