For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjustment Lock Nut | 89 N·m | 66 lb ft
Adjuster Plug Lock Nut | 109 N·m | 80 lb ft
Allen or Torx Head Screw | 25 N·m | 18 lb ft
Automatic Bleed Hole Plug | 55 N·m | 41 lb ft
Auxiliary Cylinder Plug | 41 N·m | 30 lb ft
Ball Return Guide Cap Screw | 25 N·m | 18 lb ft
Bearing Adjuster | 17 N·m | 13 lb ft
Bearing Adjuster Jam Nut | 154 N·m | 112 lb ft
Cardan Joint Pinch Bolt | 62 N·m | 45 lb in
Cooler Hose Connections to Cooler Pipe | 2.5 N·m | 22 lb in
Cooler Hose Connections to Steering Gear | 28 N·m | 21 lb ft
Front Cooler Pipe Clamp Bolt | 28 N·m | 21 lb ft
Manual Bleed Screw | 3.3 N·m | 30 lb in
Poppet Adjuster Seat and Sleeve Assembly | 13 N·m | 115 lb in
Poppet Fixed Stop Screw | 55 N·m | 41 lb ft
Power Steering Pump, Caterpillar® 3126 Engine Mounting Bolt | 125 N·m | 90 lb ft
Power Steering Pump, ZF, 8.1L Engines, Mounting Bolts | 70 N·m | 52 lb ft
Power Steering Pump, ZF, 8.1L Engines, Pulley Bolt | 50 N·m | 37 lb ft
Rear Cooler Pipe Clamp Bolt | 13 N·m | 115 lb in
Relieve Valve Cap | 41 N·m | 30 lb ft
Reservoir Mounting Bolt | 28 N·m | 21 lb ft
Saginaw Steering Gear Front Mounting Bolt Nut | 450 N·m | 330 lb ft
Saginaw Steering Gear Pitman Arm Nut | 370 N·m | 275 lb ft
Sector Shaft Adjust Screw Jam Nut | 57 N·m | 42 lb ft
Special Side Cover Bolt (Lubricated) | 232 N·m | 170 lb ft
Special Side Cover Bolt (Not Lubricated) | 312 N·m | 230 lb ft
Threaded Power Steering Hose | 38 N·m | 28 lb ft
TRW Ross Steering Gear Mounting Bolt Nut | 450 N·m | 330 lb ft
TRW Ross Steering Gear Sector Shaft Adjusting Screw Jam Nut | 58 N·m | 43 lb ft
TRW Ross Steering Gear Sealing Nut | 54 N·m | 40 lb ft
Valve Housing Bolt (Lubricated) | 109 N·m | 80 lb ft
Valve Housing Bolt (Not Lubricated) | 149 N·m | 110 lb ft