For 1990-2009 cars

RPO | Description
--- | ---
AA2 | Window: Tinted, Unshaded
ANZ | Seat: Full Width
AN8 | Seat: Front Bucket, Low Back, Driver
AQQ | Seat: Passenger Air, Low Back, Vinyl
AQR | Seat: Driver Air, High Back, Vinyl
AQS | Seat; Driver Air, Low Back, Vinyl National Cush-N-Aire
AQT | Seat: Driver Air, High Back, Vinyl
AQV | Seat: Driver Air, High Back, Cloth
AQ1 | Seat: Passenger, Bucket, Low Back
ARD | Seat: Front Bucket, Low Back, Drivers, Self-Contained Air Suspension
ARE | Seat: Front Bucket, Low Back, Passenger, Self-Contained Air Suspension
ARF | Door Check, LH
ARG | Door Check, RH
ASA | Seat Front Bucket, Driver, High Back, Self Contained Air Susp.
ASE | Equipment Air Seat
AU3 | Lock Control Side Drive, Electric
AU7 | Key Common, Fleet
AWJ | Panel Trim, Front Doors
AX2 | Key Common, Vehicular Unique
A11 | Window: Tinted, All
A58 | Seat: Passenger, Auxiliary, Two
A82 | Restraint: Head
BPP | First Position Prop Hanger, BOC, Height A
BPQ | First Position Prop Hanger, BOC, Height B
BPS | First Position Prop Hanger, BOC, Height C
BPT | First Position Prop Hanger, BOC, Height D
BPU | First Position Prop Hanger, NON-BOC, Height A
BPV | First Position Prop Hanger, NON-BOC, Height B
BPW | First Position Prop Hanger, NON-BOC, Height C
BQC | Hood Fiberglass, Access Panels
BRW | First Position Prop Hanger, Forward BOC, Height A
BRX | First Position Prop Hanger, Forward BOC, Height B
BRY | First Position Prop Hanger, Forward BOC, Height C
BRZ | First Position Prop Hanger, Forward BOC, Height D
BTW | First Position Prop Hanger, Rearward BOC, Height A
BTX | First Position Prop Hanger, Rearward BOC, Height B
BTY | First Position Prop Hanger, Rearward BOC, Height C
BTZ | First Position Prop Hanger, Rearward BOC, Height D
BVB | Step, LH, Lowered 66 mm (2.6 in)
BVL | Steps LH Lowered-1 inch, Additional
BZA | Steps LH CAB Entry and Component Box, Lowered
BZC | Steps, RH, Lowered 66 mm (2.6 in)
CC4 | Roof: Raised
CD4 | Wiper System: Windshield, Pulse
CKD | Vehicle completely Knocked Down
CRI | Equipment Uplevel Crew Cab Trim
CRW | Equipment Crew Cab
CUP | Fire Extinguisher 2.75 lb or Equivalent
C95 | Lamp: Interior, Roof, Courtesy, and Dual Reading
DC9 | Mirror O/S LH and RH, Wide Load, l Remote Control, Electric Heated, Stainless Steel, with /Clearance Lamps
DFO | Mirror: Outside, LH and RH, 17.8x40.6 cm (7x16 in), SST
DF2 | Mirror O/S LH and RH, Wide Load, Folding, Stainless Steel
DNA | Mirror: Outside, Dual West Coast Type Mirrors, Stainless Steel, Clearance Lights, 15.2x40.6 cm (6x16 in)
DNF | Mirror: Outside, Auxiliary, 127 mm (5 in) Spot, Dual, Delbar
DNN | Mirror: Outside, Dual Velvac® Heated, 15.2x40.6 cm (6 x 16 in), Stainless Steel
DPB | Mirror: Outside Dual, West Coast Type, Convex, 17.8x40.6 cm (7x16 in), Painted
DPK | Mirror O/S Dual, Velvac, SST, With Convex Lower Head.
DTE | Mirror: Auxiliary Outside, 20.3 cm (8 in) Spot, Dual, Retractable, SST
DTG | Mirror Auxiliary Outside, Sprague Multi-Vex Painted
D21 | Sunshade Windshield
D36 | Mirror: Inside Rearview, Tilt
ED1 | Wheelbase 136 inch
ED3 | Wheelbase 211 inch
ED7 | 551 cm (217 in) Wheelbase
EG4 | Wheelbase 157 inch
EK1 | Wheelbase 181 inch
EL4 | 490 cm (193 in) Wheelbase
EL8 | 500 cm (197 in) Wheelbase
EM1 | Wheelbase 199 inch
EP7 | Wheelbase 223 inch
EP9 | Wheelbase 225 inch
EQ4 | Wheelbase 229 inch
ERA | Second Position Prop Hanger, Height A
ERB | Second Position Prop Hanger, Height B
ERC | Second Position Prop Hanger, Height C
ER7 | 612 cm (241 in) Wheelbase
ES2 | 622 cm (245 in) Wheelbase
ET1 | Wheelbase 253 inch
ET7 | 658 cm (259 in) Wheelbase
EV3 | Wheelbase 273 inch
EV9 | Suspension: Attach Bolted
EW2 | Wheelbase 281 inch
EY1 | Yoke: Propeller Shaft, Driveline, Dana®
E28 | Handle Assist
FD0 | Frame: Rail, Full Depth, 612x15 cm (241x6 in), 22680 kg (50,000 lb)
FD5 | Frame: Rail, Full Depth, 622x20 cm (24x8 in), 36288 kg (80,000 lb)
FF1 | Hub: Front, Oil-Filled
FH4 | Axle: Front, 7258 kg (16,000 lb)
FK9 | Suspension Front 4090 KG Multileaf
FL1 | Axle: Front, 3674 kg (8,100 lb)
FL2 | Axle: Front, 4 990 kg (11,000 lb)
FL3 | Axle: Front, 6 623 kg (14,600 lb)
FM0 | Suspension: Front, Multileaf, 6 623 kg (14,600 lb)
FM1 | Suspension Front 18000 lb, Multileaf
FNE | Equipment H.D. Frame Crossmember (Taperleaf RR Suspension)
FNV | 445 cm (175 in) Wheelbase
FN0 | Suspension: Front, Taperleaf, 4 989 kg, (11,000 lb)
FPC | Equipment Front GVW Rating (16000#)
FPJ | 338 cm (133 in) Wheelbase
FPO | Wheelbase 163 inch
FPP | Wheelbase 163 inch
FPQ | Wheelbase 203 inch
FQX | Wheelbase 145 inch
FRP | Wheelbase 235 inch
FSA | Reinforcement Frame O/S, Inv L Type, 80K, Extended
FSC | Reinforcement Frame, O/S, Invert L Type, 110K, Extended
FSD | Axle: Front 14600 LB
FSE | Stop Bump, Front Axle
FSG | Extension Brackets, Front Bumper, 2 inch
FSJ | Extension Brackets, Front Bumper, 5 inch
FSK | Equipment Restricted Front Axle Turn
FS7 | Axle: Front, 5 443 kg (12,000 lb) HD
FUC | Frame: Extension, 61 cm (24 in) Integral Front
FWN | 475 cm (187 in) Wheelbase
F02 | Frame: Rail, Full Depth, 696x25 cm (274x10 in), 49 896 kg (110,000 lb)
F08 | Reinforcement: Frame, Outside, Inverted L Type, 36 288 kg (80,000 lb)
F12 | Suspension: Front, Tapered Leaf, 3 175 kg (7,000 lb)
F14 | Suspension: Front, Tapered Leaf, 3 674 kg (8,100 lb)
F15 | Suspension: Front, Tapered Leaf, 4 082 kg (9,000 lb)
F20 | Reinforcement: Frame, Outside, Inverted L Type, 49 896 kg (110,000 lb)
F26 | Suspension: Front, Tapered Leaf, 5 443 kg (12,000 lb)
F28 | Suspension: Front, Multileaf, 7 258 kg (16,000 lb)
F39 | Suspension: Front, Tapered Leaf, 2 654 kg (5,850 lb)
F59 | Stabilizer Shaft: Front
GG0 | Suspension: Rear, Multileaf, 6 804 kg (15,000 lb)
GG7 | Suspension: Rear, Tapered Leaf 7 666 kg (16,900 lb)
GG8 | Spring: Rear Auxiliary, Multileaf, 2 041 kg (4,500 lb)
GJ4 | Axle: Rear, 11 794 kg (26,000 lb), Eaton® 26085T, Two Speed
GNS | Suspension: Rear, 18 144 kg (40,000 lb), Hendrickson RT400
GN0 | Suspension: Rear, Multileaf, 8 618 kg (19,000 lb)
GN1 | Stabilizer Shaft: Rear
GN2 | Suspension: Rear, Tapered Leaf, 8 618 kg (19,000 lb)
GN8 | Suspension: Rear, Multileaf, 9 526 kg (21,000 lb)
GPG | Vehicle: Low Profile Package
GPL | Suspension Rear 40, 000 LB, Hend RS400, Rubber Bushing, 52 inch Beam
GPN | Vehicle Garbage Packer
GP0 | Suspension: Rear, Tapered Leaf, 10 433 kg (23,000 lb)
GPR | Suspension Rear Hendrickson RTE400, 40000# CAP, 52 inch Beams W/Bronze Center Bushing
GP1 | Suspension: Rear, Multileaf, 10 660 kg (23,500 lb)
GP9 | Suspension: Rear, Taperleaf, 8 097 kg (17,850 lb)
GQB | Third Position Prop Hanger, Height A
GQC | Third Position Prop Hanger, Height B
GQD | Third Position Prop Hanger, Height C
GQ3 | Suspension: Rear, Multileaf, 14 062 kg (31,000 lb)
GRW | Grille: Radiator Mounted
GR9 | Suspension: Rear, Tapered Leaf, 9 526 kg (21,000 lb)
GSA | Suspension: Rear, 20 866 kg (46,000 lb), Hendrickson RT460
GSD | Suspension: Rear 40,000 LB, Hend RTE400 18, 200 KG, Rubber Bush, 6 inch Beams
GSH | Suspension: Rear, 132 cm (52 in) Beam, 15 422 kg (34,000 lb), Hendrickson U340
GSJ | Suspension Rear 21,000 LB, Air
GYN | Suspension Rear 23,000 lb Capacity, Radius Leaf
GZG | GVW Rating 19,500 lb
GZH | Suspension Rear 12,000 lb, Tapered Leaf
GZI | GVW Rating: 11 771 kg (25,950 lb)
GZJ | GVW Rating: 8 165 kg (18,000 lb)
GZK | Suspension Rear Hend RT400, 40,000 lb, Rub Bush, 52 inch Beam, w/Trans Torque Rods
GZL | GVW Rating 19,800 lb.
GZM | GVW Rating 16,950 lb
GZT | Provisions for Taperleaf/Multileaf Rear Springs
G12 | Suspension Rear Air 12,000 lb
G40 | Suspension: Rear Air, 8 618 kg (19,000 lb)
G45 | Suspension Rear Air, 23,000 lb
G60 | Spring: Rear, Auxiliary
G68 | Shock Absorbers: Rear, Heavy Duty
G86 | Axle: Limited Slip
G98 | Seal: Rear Axle Oil, Stemco®
HNA | Axle: Rear, Eaton® 23105S, Single Speed, 10 433 kg (23,000 lb)
HNG | Axle Rear Eaton 23431 Single Speed, 23,000 lb CAP
HPA | Axle: Rear, Eaton® 26105S, Single Speed, 11 794 kg (26,000 lb)
HPD | Axle: Rear, Eaton® DS454P, Single Speed, 20 412 kg (45,000 lb)
HPE | Axle: Rear, Eaton® DS404, Single Speed, 18 144 kg (40,000 lb)
HPG | Axle: Rear, Eaton® 22060S, Two Speed, 9 979 kg (22,000 lb)
HPH | Axle: Rear, Eaton® 22060T, Two Speed, 9 979 kg (22,000 lb)
HPI | Axle: Rear, Eaton® DS344, Single Speed, 15 422 kg (34,000 lb)
HPJ | Axle: Rear, Eaton® DS344, Two Speed, 15 422 kg (34,000 lb)
HPK | Axle: Rear, Eaton® 19000, Two Speed, 8 618 kg (19,000 lb)
HPL | Axle: Rear, Eaton® 19060D, Single Speed, 8 618 kg (19,000 lb)
HPM | Axle: Rear, Eaton® 19060T, Two Speed, 8 618 kg (19,000 lb)
HPN | Axle: Rear, Eaton® 21060T, Single Speed, 9 526 kg (21,000 lb)
HPP | Axle: Rear, Eaton® 21060S, Single Speed, 9 526 kg (21,000 lb)
HPQ | Axle: Rear, Eaton® 23080S, Single Speed, 10 433 kg (23,000 lb)
HPZ | Control: Rear Axle Shift, Two Speed, Electric
HR1 | Control: Rear Axle Shift, Full Air, I/P Mounted
HR2 | Control Rear Axle Shift, Full Air, Trans LVR Mounted.
HVQ | Axle Rear 26,000 lb, EATON 26080P
HXB | Axle: Rear, Eaton® 19060S, Single Speed, 8 097 kg (17,850 lb)
HXC | Axle: Rear, Eaton® 1060S, Single Speed, 7 666 kg (16,900 lb)
HZZ | Provisions RR Axle Diff Lk
H08 | Axle: Rear, Dana® S150-S, Single Speed, 6 804 kg (15,000 lb)
H10 | Axle: Rear, Eaton® 15040S, Single Speed, 6 804 kg (15,000 lb)
H14 | Axle: Rear, Rockwell RS-23160, Single Speed, 10 433 kg (23,000 lb)
H15 | Axle: Rear, Eaton® 21060T, Two Speed, 9 526 kg (21,000 lb)
H17 | Axle: Rear, Eaton® 19050T, Two Speed, 8 616 kg (19,000 lb)
H20 | Axle: Rear, Eaton® 23080T, Two Speed, 10 433 kg (23,000 lb)
JE3 | Brake: Hydraulic
JE4 | Brake: Air
JE5 | Braking System: Antilock
JNC | Equipment: Four Piston Rear Disc Brakes
JNM | Cord Drain Valve
JNW | Equipment RR Brake Chamber Brand Ancorloc Life Seal
JNX | Valve: Tractor Parking Brake Control
JPT | Tank Air, Relocate, RH Side
JPV | Brake Rating: Rear, Air Carlisle, NAB9ML, Non-Asbestos Lining, 14 cm (5.5 in) Slack, 42x178 cm (16.5x7 in) Fab Shoe, 16 Hole Mounting
JPX | Tank Air, Relocate, Beverage Special
JPZ | Valve: Air Suspension, Air Release
JQB | Universal Joint: Main, 1480/148N Series
JQF | Adjuster: Rear Slack, Automatic, Rockwell®
JQJ | Joint Customer Preference Universal
JQM | Universal Joint: Main, 1710/17N Series
JQN | Universal Joint: Inter-Axle, 1710/17N Series
JQP | Universal Joint: Main, 1550/155N Series
JQQ | Universal Joint: Main, 1710/17N Series, HD Tube
JQR | Universal Joint: Main, 1610/161N Series
JQT | Equipment RR Brake Chamber Brand, MGM (Model TR-TS)
JQZ | Brake Rating: Front, Air Abex, 931-162 Non-Asbestos Lining, 14 cm (5.5 in) Slack, 42 cm x 15 cm (16.5 in x 6 in) Fab Shoe, 8 Hole Mounting
JRA | Universal Joint: Inter Axle, 1610/161N Series
JRC | Provisions Brake Adjusters - Lube for Life
JRF | Shield: Rear Brakes, Dust
JRG | Brake Rating Frt Air Abex 197, Non-Asbestos Lining 5.5 in) Slack 15 x 4, Fab shoe & 4 or 8 hole mtg
JRH | Brake rating Frt Air Abex 197, Non-Asbestos Lining, 5.5 in) Slack 16.5x5, Fab. Shoe & 8 hole mtg.
JRI | Brake Rating RR Air Abex 197, Non-Asbestos Lining ,5.5 in) Slack 16.5x7, Fab. Shoe, 10 hole mtg
JRJ | Brake Rating: Rear, Air Carlisle, NAB456, Non-Asbestos Lined, 15 cm (6 in) Slack, 42x18 cm (16.5x7 in) Cast Shoe, 16 Hole Mounting
JRO | Brake Rating RR Air ABEX 197, Non-Asbestos Lining, 5.5 in Slack 16.5x7, Fab. Shoe, 16 Hole MTG
JRW | Guards Propshaft
JTF | Brake Adjuster Front Slack, Rockwell® Manual
JTG | Brake Adjuster Rear Slack, Rockwell® Manual
JTJ | Brake Adjuster RR Slack, Eaton Automatic
JTK | Brake Adjuster: Front Slack, Eaton® Automatic
JTM | Tank Air, Relocate, Under Cab
JTT | Air Dryer B/W Model, AD9 Heated, Brake Air Tank
JTU | Air Dryer Heated, Brake Air Tank, Premium
JUE | Brake Adjuster: Front Slack, Rockwell® Automatic
JUZ | Equipment RR Brake Chamber Brand, MGM E-Series
JVA | Provisions Antilock Brake Delete
JXD | Joint: Main, 1750/176N Series, Heavy Duty Tube
JXG | Valve: Air Brake Moisture Ejector, B/W DV2, Heated, Front
JYV | Brake Provisions Full Trailer
JZC | Chamber: Front Brake, Type 16
JZD | Chamber: Front Brake, Type 20
JZE | Chamber: Front Brake, Type 24
JZF | Chamber: Rear Brake, Type 30
J69 | Parking Brake: Mechanically Operated, Lok
J71 | Parking Brake: Power Operated
J78 | Valve: Moisture Ejector Air Brake
J82 | Valve: Front Air Brake, Limiting
J91 | Brake Provisions: Trailer
KA2 | Heater Engine Block, Phillips 115V, 1500 Watt
KA4 | Engine Coolant Heater: 120V, 1000 Watt W/Cord
KC1 | Filter: Oil, Luberfiner 750C
KG3 | Generator: 145 AMP
KG8 | Generator: 130 AMP
KNB | Air Cleaner: Dry
KPJ | Engine Shutdown: Automatic
KPS | Oil Cooler: Engine
KQR | Starter: HD, Overcrank Protection
KRG | Air Cleaner: Dry Inside Type
KRW | Hose: Radiator, Silicone
KTE | Injector: Ether, Start System
KUK | Separator Fuel/Water- Racor, Cold Weather, Non- Heated
KUM | Provisions: Receptacle, Component Box
KUN | Separator, Fuel/Water, Davco, Heated, 200 Series
KUS | Air Cleaner: Dual Element
KUV | Air Compressor B/W, 13.2 CFM, Water Cooled for Accessory Drive
KUW | Fan Clutch Drive-Cold Weather
KVB | Hose: Water, Silicone, Except Radiator
KW1 | Generator: 160 AMP
KYG | Air Intake: Air Compressor Plumbed to Engine Air Cleaner
KYR | Governor: Vehicle Speed, 105 km/h (65 mph)
KYY | Joint Manifold Intake Vacuum
KZW | Valve Air Introduction Diverter
KZX | Air Compressor: B/W, 13.2 CFM, Water Cooled
K05 | Heater: Engine Coolant
K28 | Filter: Fuel
K34 | Cruise Control: Automatic, Electronic
K40 | Engine Brake: Exhaust
K53 | Fuel Sender Robust Fuel system
K60 | Generator: 100 AMP
K67 | Starter engine, Heavy Duty
K68 | Generator: 105 AMP
LG5 | Engine: 7.2l, GL, Turbo
L18 | Engine: Gas 8 Cyl, 8.1 L, MFI
MB2 | Plug: Transmission, Magnetic Filler
ME3 | Transmission: Allison® MT643D, Automatic
ME5 | Transmission: Allison® MT653DRD, Automatic
MF1 | Transmission: Allison® AT545, Automatic
MK0 | Transmission: Manual, 5-Speed, Eaton®, 7.22 1st, 1.39 4th, Direct Drive
MK8 | Transmission: Manual, 7-Speed, Spicer, ES52-7B 10.09 1st, Direct Drive
MK9 | Transmission: Manual, 5-Speed, Eaton®, 7.22 1st, 1.27 4th, Direct Drive
ML0 | Transmission: Eaton® FS6105B, Manual 5-Speed
mm7 | Transmission Manual 6 Speed Eaton BOOS SYNC, 9.01 1ST, 560 lb ft Direct Drive
mm8 | Transmission Manual 6 Speed, Eaton BOOS SYNC, 9.01 1ST, 660 lb ft Direct Drive
MNC | Transmission: Manual, 5-Speed, Eaton®, 6.82 1st, 4th, Direct Drive
MNK | Transmission 5 Speed Automatic Allison, MD3060P W/PTO, Drive Gear
MNZ | Transmission: Allison MD3560P W/PTO, 5-Speed Automatic
MPD | Kit Shift Modify, 3RD Gear Hold
MPJ | Clutch, Cerametallic, 33 cm (13 in), Eaton® Valeo
MPK | Clutch 14"-2 Ceramic Pull Type Greasable Bearing
MPU | Transmission: Eaton® FS5005A, Manual, 5-Speed
MP8 | Transmission: Allison® MD3060P W/PTO, Automatic
MSC | Transmission: Eaton® FS4005B, Manual, 5-Speed
MSG | Transmission: Eaton® FS4005A, Manual, 5-Speed
MS9 | Transmission Manual 5 Speed, Eaton, 8.05 1st, D/Drive
MTA | Provisions: Fire Truck W/Split Shaft PTO
MTD | Clutch: 14-1 Cerametallic, Eaton-Valeo®, Pull Type
MTG | Provisions: Fire Truck W/Split Shaft
MTJ | Provisions: Fire Truck W/Split Shaft PTO
MTK | Provisions Refuse Trk, Auto Neutral
MTO | Cable Clutch-Felsted
MTP | Transmission: Allison® MD3560P W/PTO, Automatic
MTW | Transmission Automatic 5 Speed, Allison, LCT 2400, W/PTO Drive Gear and Park Pawl
MT3 | Transmission Manual 10 Spd, Eaton RT8908LL, D/Drive
MUQ | Control Shift: Automatic Transmission, Steering Column Mounted
MUR | Control Shift: Automatic Transmission, I/P Mounted
MUT | Transmission Manual 9 Speed, Eaton® RT6609, Direct Drive
MUY | Provisions Sewer Cleaning Truck
MUZ | Transmission Oil Filter
MWE | Pilot Shaft: Automatic Transmission, No Spline
MWF | Pilot Shaft: Automatic Electric Transmission, No Spline
MWM | Clutch Spicer® 14-1 Cerametallic Pull Type Greasable Bearing
MWW | Pilot Shaft Transmission, 44.45 mm (1.75 in) Spline
MWX | Pilot Shaft: Transmission, 38.1 mm (1.5 in) Spline
MXD | Provisions Lubrication, Clutch
MX4 | Transmission Auto 5 SPD, Allison, LCT 2000, 3.51 1st, 1.00 4th 0.73 5TH, O/D, CONV Clutch
MZE | Clutch: 35.6 cm (14 in) - 2 Pull Type, Cerametallic
M69 | Transmission Manual 6 Spd, Eaton, FS08306, 6.62 1st, O/D
NB5 | Exhaust System: Single
ND5 | Fuel Tank: 189L (50 Gal), LH, Rectangular Step
NE5 | Fuel Tank: 189L (50 Gal), RH, Rectangular Step
NE6 | Fuel Tank: 189L (50 Gal), Dual Rectangular Step
NJ2 | Fuel Tank: Temporary
NM8 | Leaded Fuel System: Compatible
NPD | Rain Cap: Exhaust Stack
NPT | Exhaust System: Single Horizontal Muffler w/Vertical Tailpipe, Right Hand Cab Mounted
NPY | Exhaust System: Single Horizontal Muffler w/Vertical Tailpipe, Left Hand Cab Mounted
NP5 | Steering Wheel: Leather Wrapped
NQC | Fuel Tank: 132.5 L (35 Gal), 28x61 cm (11x24 in), Dual Rectangular, Integral Step
NRZ | Exhaust Emission Control: Diesel, W/O Converter
NWB | Separator: Racor Spin-On, Fuel/Water
NWD | Exhaust Modification, Increased Ground Clearance
NWE | Fuel Tank RH RECT 35 GAL, 25x15, Includes Step
NWR | Cab Reinforcements-Dual Vert Exhaust
NXM | Fuel Additional-10 Gallons
NXN | Fuel: 57 L (15 Gal) Additional
NXW | Steering: Power, Midland Ross
N33 | Steering Column: Tilt Type
N40 | Steering: Power, Non-Variable Ratio
PNB | Wheel: Polished Aluminum, Both Sides, Rear
PNQ | Angle: Rear Axle Pinion, Nominal 3°
PNR | Angle: Rear Axle Pinion, Nominal 4°
PNS | Angle: Rear Axle Pinion, Nominal 5°
PNX | Angle: Rear Axle Pinion, Nominal 6°
PNY | Angle: Rear Axle Pinion, Nominal 7°
PQA | Wheel: Front, Generic Aluminum/Thick Disc Slt, 10 Hole, 287.75 mm (11.25 in) BC BS, Disc
PQB | Wheel: Front, Generic Steel, 10 Hole, 287.75 mm (11.25 in) BC BS, Disc
PQC | Wheel: Rear, Aluminum, 10 Hole Disc, 287.75 mm (11.25 in) BC BS
PQD | Wheel: Rear, Generic Steel, 10 Hole Disc, 11.25 BC BS
PQJ | Wheel: Front, Cast, 20 x 22.5
PQK | Wheel: Rear, Cast, 20 x 22.5
PQN | Tank Fuel, Natural Gas, 76 L (20 Gal) Equivalent
PQR | Wheel: Front Generic, 8 Hole, 275 mm (10.8 in), BC, FN
PQS | Wheel: Rear Generic, 8 Hole Disc, 275 mm (10.8 in) BC, FN
PQU | Wheel: Front, Generic Steel, 10 Hole, 287.75 mm (11.25 in), BC Piloted, Disc
PQV | Wheel: Rear, Generic Steel, 10 Hole, 287.75 mm (11.25 in), BC, Piloted, Disc
PQY | Wheel: Front, Generic Steel, 10 Hole, 287.75 mm (11.25 in), BC, Piloted
PQZ | Wheel: Rear, Generic Steel, 10 Hole, 287.75 mm (11.25 in), BC, Piloted
PST | Color: Var. 1, Two-Tone, Scheme Z
PTO | Provisions Power Take Off Controls
PVA | Paint Process Wheels, Pre-Painted, White
PVB | Fuel Tank: RH, 227 L (60 Gal), Integral Step
PVC | Fuel Basket, Anti-Syphon
PVE | Fuel Tank 227 L, 60 Gal, LH, Rect. 25 x 15, INT Step
PVG | Wheel Front Generic 8 Hole, 275 mm BC FN Alum/Thick Disc
PVH | Wheel Rear Generic 8 Hole, 275 mm BC FN Alum/Thick Disc
PVM | Tank Fuel, Natural Gas, 3600 PSI, 30 Equivalent Gallon Gasoline Capacity
PVP | Paint Process Wheels, Pre-Painted, White Powder Coat
PZB | Fuel Tank: LH, Rectangular, Step, 133 L (35 Gal)
P50 | Tires Customer Property, Front
P51 | Tires Customer Property, Rear
P52 | Tires Customer Property, Spare
P53 | Tire Tread, Spare Tread and Brand, Front Match
P54 | Tire Tread, Spare Tread and Brand, Rear Match
QA5 | Wheel: Front, 22.5x9.0, 10 Stud, 287.75 mm (11.25 in) BC BS Type MTG, 3.75 Offset
QE5 | Odometer Rear Axle Hub
QH3 | Wheel: Front, 22.5x7.50, 10 Hole, 287.75 mm (11.25 in) BC, FN, Hub Piloted
QH4 | Wheel: Rear, 22.5x7.50, 10 Hole, 287.75 mm (11.25 in) BC, FN, Hub Piloted
QH8 | Wheel: Front, 22.5x9.00, 10 Hole, 287.75 mm (11.25 in) BC, FN, Hub Piloted
QJ3 | Wheel: Front, 20x8, 5° Rim
QJ4 | Wheel: Rear, 20x8, 5° Rim
QK1 | Wheel: Front, 20x7.5, 5° Rim
QK2 | Wheel: Rear, 20x7.5, 5° Rim
QM1 | Wheel: Front, 22.5x7.5, Rim DCT
QM2 | Wheel: Rear, 22.5x7.5, Rim DCT
QM6 | Wheel: Front, 22.5x8.25, Rim DCT
QM7 | Wheel: Rear, 22.5x8.25, Rim DCT
Q21 | Wheel Spacer Rear, 4 inch
Q8C | Cap Valve, Tire, Air-Thru
Q8D | Mud Flaps Front
Q8G | Mud Flaps Front-Extended
Q82 | Wheel: Front, 19.5x6.0, 8 Hole, 275 mm (10.8 in), BC, FN
Q83 | Wheel: Rear, 19.5x6.0, 8 Hole, 275 mm (10.8 in), BC, FN
Q86 | Wheel Front 22.5x8.25, 10 Hole, 285.75 mm BC, Piloted Hub - Accuride 28408
Q87 | Wheel Rear 22.5x8.25, 10 Hole, 285.75 mm BC, Piloted Hub - Accuride 28408
RHL | Wheel: Front, 22.5x9.0. Rim DCT
RLE | Wheel: Front, 22.5x7.5, 10 Hole, 287.75 mm (11.25 in) BC, BS, DCT, BAL, (FI-27403)
RLF | Wheel: Rear, 22.5x7.5, 10 Hole, 287.75 mm (11.25 in) BC BS, DCT, BAL, (FI-27403)
RNB | Wheel Front 24.5x8.25, 10 Hole, 285.75 mm BC Piloted Hub Alum (Accuride 29137)
RNH | Wheel Front 22.5x8.25, 10 Hole, 285.75 mm BC Piloted Hub Aluminum (AKW RA29555)
RNN | Wheel RR 22.5x8.25, 10 Hole, 285.75 mm BC Piloted Hub Aluminum (AKW RA29555)
RNP | Wheel Front 24.5x8.25, 10 Hole, 285.7 mm BC, Piloted Hub (Accuride 28641)
RNQ | Wheel Rear 24.5x8.25, 10 Hole, 285.7 mm BC, Piloted Hub (Accuride 28641)
RPF | Wheel Front 22.5x8.25, 10 Hole, 11.25 BC BS DCT
RPG | Equipment Wheel and Drum, 6 Spoke 20 inch Cast
RPM | Wheel Front 19.5 x 6.75, 8 Hole 275 mm BC FN, 5.55, Offset, Alcoa Alum
RPQ | Wheel: Front, 22.5x8.25, 10 Hole, 285.75 mm (11.25 in) BC, Piloted Hub
RPR | Wheel: Rear, 22.5x8.25, 10 Hole, 285.75 mm (11.25 in) BC, Piloted Hub
RPS | Wheel Front 22.5x7.5 10 Hole 11.25 BC BS DCT ALM (Accuride)
RPT | Wheel Rear 22.5x7.5 10 Hole 11.25 BC DCT ALM (Accuride)
RPW | Wheel Rear 19.5x6.75, 8 Hole 275 mm BC FN, 5.55, Offset, Alcoa Alum
RQ2 | Vehicle Application: Truck Service
RQ3 | Vehicle Application: Truck-Tractor Service
RRS | Wheel: Front, 22.5x8.25, 10 Hole, 285.75 mm (11.25 in) BC BS, DCT, (FI-27404)
RRT | Wheel: Rear, 22.5x8.25, 10 Hole, 285.75 mm (11.25 in) BC, BS, DCT (FI-27404)
R3B | Front Tire: Extra Strength Highway Tread
R3C | Front Tire: Premium Highway Tread
R3D | Front Tire: Premium Highway Tread
R3E | Front Tire: Highway Off-Road
R3F | Front Tire: Off-Road Tread
R3H | Front Tire: Highway Traction Tread
R3J | Front Tire: Highway Traction Block Tread
R3K | Front Tire: On/Off Road Rib Tread
R3L | Front Tire: Off-Road Traction Tread
R3M | Front Tire: All Season Tread
R3N | Front Tire: Premium Highway Improved Steering Control Tread
R3S | Tire Tread Front Highway RIB-XRV
R3T | Tire Tread Front On/Off Road Traction-Directional
R4A | Front Tire Brand: Goodyear
R4H | Front Tire Brand: General
R4L | Front Tire Brand: Michelin
R4N | Front Tire Brand: Bridgestone
R4R | Front Tire Brand: Select, Brand Plant
SGA | Wheel: Additional, Rear Spare
SMA | Spacer Pack: Right Spring Cab Leveling, +10 mm (+0.374 in)
SMB | Spacer Pack: Right Spring Cab Leveling, +0 mm (+0 in)
SMC | Spacer Pack: Right Spring Cab Leveling, -10 mm (-0.374 in)
SMD | Spacer Pack: Right Spring Cab Leveling, -20 mm (-.787 in)
SNF | Wheel: Front, Spare
SNR | Wheel: Rear, Spare
SRV | Tires, Additional Rear Spare
SVA | Holder Cup
S3B | Tire Tread: Rear, Extra Strength Highway
S3C | Tire Tread: Rear, Premium Highway
S3D | Tire Tread: Rear, Highway Premium
S3E | Tire Tread: Rear, On/Off Road Highway
S3F | Tire Tread: Rear, Off Road Rolling
S3H | Tire Tread: Rear, Highway
S3J | Tire Tread: Rear, Highway Traction
S3K | Tire Tread: Rear, On/Off Road Rib
S3L | Tire Tread: Rear, Off Road Traction
S3M | Tire Tread: Rear, All Season
S3P | Tire Tread Rear Highway Traction-Directional
S3R | Tire Tread Rear Highway Traction-Directional
S3S | Tire Tread Rear Highway RIB-XRV
S3T | Tire Tread Rear On/Off Road Traction-Directional
S4A | Rear Tire Brand: Goodyear
S4C | Rear Tire Brand: Dunlop
S4H | Rear Tire Brand: General
S4L | Rear Tire Brand: Michelin
S4N | Rear Tire Brand: Bridgestone
S4R | Rear Tire: Select, Brand Plant
S4T | Rear Tire Brand: Yokohama
TM0 | Battery: Dual
TM1 | Battery: Single
TM2 | Battery: Single, Delco® Freedom
TNL | Battery: Twin, 12V (1110)
TNN | Battery: Twin, Delco® 1150, 12V
TNQ | Battery: Delco® 1150
TNR | Battery: Three, Delco® 1150, 12V
TPL | Battery: 750 CCA, Delco® 1110
TRF | Tires: Front, Radial Identifier
TRG | Tire Selection, Customer Brand
TRH | Tire Selection, Customer Brand
TRR | Tires: Rear, Radial Identifier
TRZ | Equipment Air Shift Transmission
T40 | Hood Sloped
T50 | Hood Special Application
UEJ | Provisions Battery Positive Aux Feed
UEK | Switch, Hazard Warning
UEP | Provisions, Jump Start Aid
UER | Equipment: Tachometer and Engine Alarm
UET | Indicator, Electronic Transmission, Oil Level
UF3 | High Idle Switch
UH2 | Indicator: Seat Belt Warning
UM6 | Radio: AM/FM Stereo, Seek & Scan, Auto Rev Cassette, Clock, ETR
UM7 | Radio: AM/FM Stereo, Seek & Scan, Clock, ETR
UNE | Switch Transmission Interlock
UNK | Provisions Anti-Lock Brake Wiring Harness (Additional 6 Ft Length)
UPM | Gage: Filterminder, Air Cleaner Restriction, Dash Mounted
UUE | Horn: Air, Single Dual Trumpet
UWK | Wiring Provisions Body Marker Lamp
UXB | Wiring Harness: Trailer, 7-Wire, Generic
UXQ | Gage: Metric package
UXT | Gage: Transmission Temperature
UXZ | Radio Provisions
UZF | Alarm B/U Electrical, 97 Decibels
U08 | Horn: Dual Electric
U16 | Tachometer: Engine
U37 | Lighter: Cigarette
U86 | Wiring Harness: Full Trailer, 7-Wire
VB5 | Bumper: Front, Painted, Plastic End Caps
VCD | Provisions Battery Taper Post
VCE | Provisions Tail Lamp
VCF | Provisions Engine Tachograph
VCG | Provision International switch/control symbols
VCH | Provision Jack & Fire Extinguisher
VCI | Provisions Vehicle ID Plate
VCK | Provisions Test Ports-Air Brake System
VH4 | Mud Flaps
VPG | Cable: Trailer Jumper Cable , 7-Wire, 12-foot, Synflex Coiled
VQB | Bumper: Front, Swept Back Channel
VWN | Hook: Tow, Rear, Bolt On
VXF | Vehicle Fire Fighting
V01 | Radiator: Heavy Duty
V04 | Shutters, Radiator
V10 | Provision Options: Cold Climate
V14 | Transmission: Cooler Oil
V46 | Bumper: Chrome, Front
V66 | PTO: Provisions For
V71 | Plate inscription Series 6500
V72 | Plate Inscription Series 5500
V74 | Plate inscription Series 7500
V75 | Plate Inscription Series 8500
V76 | Hook: Tow
WHX | Reinforcement Frame O/S, INVL, Special 80K
XRL | Tire: Front, 235/80R22.5/G, 14PR, BL TL Radial
XRN | Tire: Front, 295/75R22.5/G, 14PR, BL TL Radial
XRV | Tire: Front, 285/75R24.5/G, 14PR, BL TL Radial
XSB | Tire: Front, 255/80R22.5/G, 14PR, BL TL Radial
XSH | Tire: Front, 275/80R24.5/G, 14PR, BL TL Radial
XSJ | Tire: Front, 275/80R24.5/G, 14PR, BL TL Radial
XSK | Tire: Front, 295/80R22.5/H, 16PR, BL TL Radial
XSL | Tire: Front,275/80R22.5/H ,16PR, BL TL Radial
XTB | Tire; Front 255/70r22.5/H, 16PR BL TL Radial
XTI | Tire: Front, 245/70R19.5/F, 12PR, BL TL Radial
XTN | Tire: Front, 225/70R19.5/F, BW, R/ST TL HWY
XTQ | Tire: Front, 245/75R22.5/G, BL TL Radial
XTU | Tire: Front, 265/75R22.5/G, BL TL Radial
XTY | Tire: Front, 245/70R19.5/G, 14PR, BL TL Radial
XUE | Tire: Front, 9.00R22.5/G, 12PR, BL Radial TL
XUN | Tire: Front, 9.00R20.0/F, 12PR, BL Radial TT
XWH | Tire: Front, 10.00R20/G, 14PR, BL Radial TT
XWJ | Tire: Front, 10.00R22.5/F, 12PR, BL Radial TL
XWK | Tire: Front, 10.00R22.5/G, 14PR, BL Radial TL
XWL | Tire: Front, 11.00-R22.5/G, 14PR, BL Radial TL
XWM | Tire: Front, 11.00R22.5/H, 16PR, BL Radial TL
XWN | Tire: Front, 315/80R22.5/J, 18PR, BL Radial TL
XWP | Tire: Front, 12.00R22.5/H, 16PR, BL Radial TL
XWR | Tire: Front, 315/80R22.5/L, 20PR, BL Radial TL
X5Z | Warranty: Engine Only, 80 450 km (50,000 mi)/3 Years
X6Y | Warranty: Engine Only, 80 450 km (50,000 mi)/4 Years
X62 | Bumper: Front, Steel Channel Type
X80 | Plate GVW Rating
X88 | Name Plate: Chevrolet
X9K | Warranty: Engine Only, 160 900 km (100,000 mi)/4 Years
YE9 | Convenience Package, Comfort and Decor
YG9 | Warranty: Engine Only, 160 900 km (100,000 mi)/5 Years
YRL | Tire: Rear, 235/80R22.5/G, 14PR, BL TL Radial
YRN | Tire: Rear, 295/75R22.5/G, 14PR, BL TL Radial
YRP | Tire: Rear, 11.00R20/H, 16PR, BL Radial TT
YRV | Tire: Rear, 285/75R24.5/G, 14PR, BL TL Radial
YSB | Tire: Rear, 255/80R22.5/G, 14PR, BL TL Radial
YSH | Tire: Rear, 275/80R24.5/G, 14PR, BL TL Radial
YSJ | Tire: Rear, 275/80R24.5/G, 14PR, BL TL Radial
YSL | Tire: Rear, 275/80r22.5-H, 16PR BL TL Radial
YTB | Tire: Rear, 255/70R22.5/H, 16PR, BL TL Radial
YTI | Tire: Rear, 245/70R19.5/F, 12PR, BL TL Radial
YTN | Tire: Rear, 225/70R19.5/F, BW R/ST ST TL HWY
YTQ | Tire: Rear, 245/75R22.5/G, BL TL Radial
YTU | Tire: Rear, 265/75R22.5/G, BL TL Radial
YTY | Tire: Rear, 245/70R19.5/G, 14PR, BL TL Radial
YUE | Tire: Rear, 9.00R22.5/F, 12/PR, BL Radial TL
YUN | Tire: Rear, 9.00R20.0/F, 12PR, BL Radial TT
YU8 | Wheel: Single, Polished Aluminum, One Side, Front
YWH | Tire: Rear, 10.00R20/G, 14PR, BL Radial TT
YWJ | Tire: Rear, 10.00R22.5/F, 12PR, BL Radial TL
YWK | Tire: Rear, 10.00R22.5/G, 14PR, BL Radial TL
YWL | Tire: Rear, 11.00R22.5/G, 14PR, BL Radial TL
YWM | Tire: Rear, 11.00R22.5/H, 16PR, BL Radial TL
YWP | Tire: Rear, 12.00R22.5/H, 16PR, BL Radial TL
YX6 | Attachment Main Driveline One-Shaft System
YX7 | Attachment Main Driveline Two-Shaft System
YX8 | Attachment Main Driveline Three-Shaft System
YX9 | Attachment Main Driveline Four-Shaft System
ZRL | Tire: Spare, 235/80R22.5/G, 14PR, BL TL Radial
ZRN | Tire: Spare, 295/75R22.5/G, 14PR, BL TL Radial
ZRP | Tire: Spare, 11.00R20/H, 16PR, BL Radial TT
ZRV | Tire: Spare, 285/75R24.5/G, 14PR, BL TL Radial
ZSB | Tire: Spare, 255/80R22.5/G, 14PR, BL Radial TL
ZSH | Tire: Spare 275/80R22.5/G, 14PR, BL Radial TL
ZSJ | Tire: Spare, 275/80R24.5/G, 14PR, BL Radial TL
ZSK | Tire: Spare, 295/80R22.5/H, 16PR, BL Radial TL
ZTB | Tire: Spare, 255/70R22.5/H, 16PR BL TL Radial
ZTI | Tire: Spare, 245/70R19.5/F, 12PR BL TL Radial
ZTN | Tire: Spare, 225/70R19.5/F, BW R/ST ST TL HWY
ZTQ | Tire: Spare, 245/75R22.5/F, BL TL Radial
ZTU | Tire: Spare, 265/75R22.5/G, BL TL Radial
ZTY | Tire: Spare, 245/70R19.5/G PR BL Radial
ZUE | Tire: Spare 9.00R22.5/F, 12PR, BL TL Radial
ZUN | Tire: Spare, 9.00-20.0/F, 12PR, BL Radial TT
ZWH | Tire: Spare, 10.00R20/G, 14PR, BL Radial TT
ZWJ | Tire: Spare, 10.00R22.5/F, 12PR, BL Radial TT
ZWK | Tire: Spare, 10.00R22.5/G, 14PR, BL Radial TT
ZWL | Tire: Spare, 11.00R22.5/G, 14PR, BL Radial TT
ZWM | Tire: Spare, 11.00R22.5/H, 16PR, BL Radial TL
ZWN | Tire: Spare, 315/80R22.5J, 18PR, BL Radial TL
ZWP | Tire: Spare, 12.00R22.5/H, 16PR, BL Radial TL
ZWR | Tire: Spare, 315/80R22.5/I, 20PR, BL Radial TL
Z88 | Conversion Name PLT GMTB
001 | 3.70 Ratio Code
002 | 4.11 Ratio Code
003 | 4.33 Ratio Code
004 | 4.78 Ratio Code
005 | 4.56 Ratio Code
006 | 4.63 Ratio Code
008 | 4.88 Ratio Code
009 | 5.29 Ratio Code
010 | 5.43 Ratio Code
011 | 5.57 Ratio Code
012 | 5.83 Ratio Code
013 | 3.73 Ratio Code
014 | 6.14 Ratio Code
015 | 6.17 Ratio Code
016 | 5.25 Ratio Code
017 | 6.50 Ratio Code
018 | 6.65 Ratio Code
019 | 6.67 Ratio Code
020 | 5.63 Ratio Code
021 | 6.83 Ratio Code
022 | 7.17 Ratio Code
034 | 3.54 Ratio Code
035 | 3.54 Ratio Code
036 | 6.57 Ratio Code
038 | 6.57 Ratio Code
039 | 3.55 Ratio Code
041 | 7.39 Ratio Code
045 | 5.91 Ratio Code
051 | 6.43 Ratio Code
057 | 3.36 Ratio Code
066 | 4.10 Ratio Code
069 | 3.90 Ratio Code
070 | 5.38 Ratio Code
071 | 3.91 Ratio Code
073 | 5.04 Ratio Code
086 | 9.08 Ratio Code
090 | 3.08 Ratio Code
092 | 4.30 Ratio Code
40P | Wheel Color White (91)
41P | Wheel Color Black (91)
5E6 | ABS Name Plate
7Y4 | Meter Engine, Hour
8M3 | Swith Dome Light, R.H. Door Operated
8M7 | Headlamps Substitution
8R8 | Fuel Filter Spin Off (SEO)
9H6 | Lamp Five, Roof Marker, Truck (SEO)