For 1990-2009 cars

Table 1: | Generator C2 (L18)
Table 2: | Generator C2 (LG5)
Table 3: | Generator Inline Fuse
Table 4: | Starter Relay
Table 5: | Starter Temperature Switch

#### Generator C2 (L18)

Connector Part Information |

• | 12186568

• | 4-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1477 | Generator Output Tachometer Pulse
B | RED | 225 | Generator Turn On Signal
C | GRY | 23 | Generator Field Duty Cycle Signal
D | RED | 442 | Battery Positive Voltage

#### Generator C2 (LG5)

Connector Part Information |

• | 12052315

• | 2-Way F Metri-Pack 630 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 442 | Fuse Output-Battery
B | BRN | 25 | Charge Indicator Lamp Output

#### Generator Inline Fuse

Connector Part Information |

• | 12066681

• | 2-Way F Metri-Pack 630 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 53 | Fuse Output Generator Tachometer Pulse Type III Fuse
B | PPL | 1477 | Generator Output Tachometer Pulse

#### Starter Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack 280 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | PPL | 6 | Starter Solenoid Crank Voltage
85 | PPL | 806 | Crank Voltage (L18)
85 | ORN/BLK | 434 | Neutral Safety Switch Signal (LG5)
86 | YEL | 447 | Starter Relay Coil Control (L18)
86 | BLK | 650 | Ground (LG5)
87 | RED | 2 | Battery Positive Voltage

#### Starter Temperature Switch

Connector Part Information |

• | 12162193

• | 2-Way F Metri-Pack 150.2 Series, Sealed, P2S (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 434 | Neutral Safety Switch Signal
B | ORN/BLK | 434 | Neutral Safety Switch Signal