For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Bracket Bolt | 9 N·m | 80 lb in
Air Compressor Bracket Bolt and Nut | 67 N·m | 49 lb ft
Camshaft Position Sensor Bolt | 12 N·m | 106 lb in
Camshaft Retainer Bolt | 12 N·m | 106 lb in
Camshaft Sprocket Bolt | 30 N·m | 22 lb ft
Connecting Rod Nut - First Pass | 30 N·m | 22 lb ft
Connecting Rod Nut - Final Pass | 90 Degrees
Coolant Crossover Pipe Bolt | 50 N·m | 37 lb ft
Coolant Drain Hole Plug - Left Front | 60 N·m | 44 lb ft
Coolant Drain Hole Plug - Sides | 30 N·m | 22 lb ft
Crankshaft Balancer Bolt | 255 N·m | 189 lb ft
Crankshaft Bearing Cap Inner Bolts - First Pass | 30 N·m | 22 lb ft
Crankshaft Bearing Cap Inner Bolts - Final Pass | 90 Degrees
Crankshaft Bearing Cap Outer Studs/Bolts - First Pass | 30 N·m | 22 lb ft
Crankshaft Bearing Cap Outer Studs/Bolts - Final Pass | 80 Degrees
Crankshaft Oil Deflector Nut | 50 N·m | 37 lb ft
Crankshaft Position Sensor Bolt | 12 N·m | 106 lb in
Cylinder Head Bolt - In Sequence

- First Pass

30 N·m

22 lb ft

- Second Pass

30 N·m + 120 Degrees

22 lb ft + 120 Degrees

- Final Pass - Long Bolts #1, 2, 3, 6, 7, 8, 9, 10, 11, 14, 16, 17

60 Degrees

- Final Pass - Medium Bolts #15, 18

45 Degrees

- Final Pass - Short Bolts #4, 5, 12, 13

30 Degrees

Cylinder Head Coolant Hole Plug | 50 N·m | 37 lb ft
Drive Belt Idler Pulley Bolt | 50 N·m | 37 lb ft
Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
EGR Cover Stud | 7 N·m | 62 lb in
EGR Cover Nut | 22 N·m | 16 lb ft
EVAP Purge Valve Bolt | 8 N·m | 71 lb in
Engine Block Heater | 50 N·m | 37 lb ft
Engine Block Oil Gallery Front Plug | 30 N·m | 22 lb ft
Engine Block Oil Gallery Side Plug | 30 N·m | 22 lb ft
Engine Block Oil Gallery Rear Plug | 30 N·m | 22 lb ft
Engine Block Oil Gallery Top Plug | 20 N·m | 15 lb ft
Engine Coolant Temperature (ECT) Sensor | 50 N·m | 37 lb ft
Engine Coolant Temperature (ECT) Sensor Bracket Bolt | 50 N·m | 37 lb ft
Engine Harness Bracket Bolt | 25 N·m | 18 lb ft
Engine Harness Clip Bolt | 12 N·m | 106 lb in
Engine Lift Bracket Bolt | 40 N·m | 30 lb ft
Engine Mount Bracket to Engine Block Bolt | 70 N·m | 52 lb ft
Engine Mount Bracket to Engine Block Nuts | 45 N·m | 33 lb ft
Engine Mount Bracket to Engine Block (M10 STUD) | 30 N·m | 22 lb ft
Engine Mount Bracket to Engine Mount Bolts | 240 N·m | 177 lb ft
Engine Mount to Frame C-Channel Bolts | 160 N·m | 118 lb ft
Exhaust Manifold - Center Bolt | 35 N·m | 26 lb ft
Exhaust Manifold Heat Shield - Bolt | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield - Nut | 25 N·m | 18 lb ft
Exhaust Manifold - Nut | 16 N·m | 12 lb ft
Exhaust Manifold - Stud | 20 N·m | 15 lb ft
Flywheel Bolt - First Pass | 40 N·m | 30 lb ft
Flywheel Bolt - Second Pass | 80 N·m | 59 lb ft
Flywheel Bolt - Final Pass | 100 N·m | 74 lb ft
Flywheel Cover Bolt | 12 N·m | 106 lb in
Flywheel Holding Tool Bolt | 50 N·m | 37 lb ft
Flywheel Housing - Hex Head Bolt | 67 N·m | 50 lb ft
Flywheel Housing - Countersunk Bolt | 60 N·m | 44 lb ft
Front Cover Bolt - First Pass | 6 N·m | 53 lb in
Front Cover Bolt - Final Pass | 12 N·m | 106 lb in
Fuel Rail Bolt/Stud | 12 N·m | 106 lb in
Ground Strap Bolt | 50 N·m | 37 lb ft
Ignition Coil Bolt | 12 N·m | 106 lb in
Ignition Coil Wiring Harness Bolt | 12 N·m | 106 lb in
Inner C-Channel to Frame Bolts | 100 N·m | 74 lb ft
Intake Manifold Bolt - In Sequence - First Pass | 5 N·m | 44 lb in
Intake Manifold Bolt - In Sequence - Second Pass | 8 N·m | 71 lb in
Intake Manifold Bolt - In Sequence - Third Pass | 12 N·m | 106 lb in
Intake Manifold Bolt - In Sequence - Final Pass | 15 N·m | 11 lb ft
Knock Sensor | 20 N·m | 15 lb ft
Knock Sensor Heat Shield Bolt | 50 N·m | 37 lb ft
MAP Sensor Bolt | 12 N·m | 106 lb in
Oil Cooler Hose Fittings | 23 N·m | 17 lb ft
Oil Cooler Line Bracket Bolt | 9 N·m | 80 lb in
Oil Fill Tube Bolt | 12 N·m | 106 lb in
Oil Fill Tube Nut | 12 N·m | 106 lb in
Oil Filter | 38 N·m | 28 lb ft
Oil Filter Fitting | 66 N·m | 49 lb ft
Oil Level Indicator Tube Nut | 18 N·m | 13 lb ft
Oil Level Sensor | 20 N·m | 15 lb ft
Oil Pan Bolt - First Pass | 10 N·m | 89 lb in
Oil Pan Bolt - Final Pass | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 28 N·m | 21 lb ft
Oil Pressure Gage Sensor | 30 N·m | 22 lb ft
Oil Pump Bolt | 75 N·m | 56 lb ft
Oil Pump Cover Bolt | 12 N·m | 106 lb in
Oil Pump Drive Bolt | 25 N·m | 18 lb ft
Spark Plug | 20 N·m | 15 lb ft
Thermostat Housing Bolt | 30 N·m | 22 lb ft
Throttle Body - Nut | 10 N·m | 89 lb in
Throttle Body - Stud | 12 N·m | 106 lb in
Transmission Converter Cover Bolts | 12 N·m | 106 lb in
Transmission Fluid Cooler Line Bracket Bolt | 30 N·m | 22 lb ft
Transmission Fluid Cooler Line Clip Bolt | 30 N·m | 22 lb ft
Valve Lifter Guide Retainer Bolt | 25 N·m | 18 lb ft
Valve Rocker Arm Cover Bolt - First Pass | 6 N·m | 53 lb in
Valve Rocker Arm Cover Bolt - Second Pass | 12 N·m | 106 lb in
Valve Rocker Arm Nut | 35 N·m | 26 lb ft
Valve Rocker Arm Stud | 50 N·m | 37 lb ft
Water Pump Bolt - First Pass | 25 N·m | 18 lb ft
Water Pump Bolt - Second Pass | 50 N·m | 37 lb ft
Water Pump Pulley Bolt | 25 N·m | 18 lb ft