ENGINE FLARE SLIPS NO DRIVE ON TURNS -84-87 THM 440T4. Chevrolet Celebrity 1985

For 1990-2009 cars

# ENGINE FLARE SLIPS NO DRIVE ON TURNS -84-87 THM 440T4

#### MODEL AND YEAR: 1984-87 CELEBRITY WITH THM 440-T4 TRANSAXLE

A condition of engine flare or transmission slippage during vehicle turns may be repaired by installing a new filter.

The filter with a new inlet and baffle design entered production April 6, 1987, (Julian date 096, Figure 1) .

Check for proper fluid level and correct, as necessary. If the flare still occurs, remove the bottom pan and replace the filter and seal with a new filter and seal package listed below.

Part Name Part Number --------- ----------- Filter and Seal Package 8646902

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.