SQUEAK NOISE AT DRIVERS SEAT TO FLOOR ATTACHMENT. Chevrolet Celebrity 1988

For 1990-2009 cars

# SQUEAK NOISE AT DRIVERS SEAT TO FLOOR ATTACHMENT

#### Model and Year: 1988 CELEBRITY WITH BUCKET OR 45/55 SEAT OPTION

The 1988 Celebrity floor pan squeak noise can be repaired by making clearance between the two possible contact points of the rear right hand bracket and floor pan of the drivers seat.

1. Remove the driver seat assembly as described in the service manual (Section 9A).

2. Remove rear seat cushion assembly and left hand side sill plate moldings to remove carpet.

3. Lift the carpet up to get access to the rear right hand seat bracket.

4. Use appropriate tool to bend burr at the trim angle to give the clearance between the seat bracket and the floor pan. (See Illustration).

Labor Operation Number: T1326

Labor Time: 0.7 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.