ENGINE ROUGH VOLTAGE SPIKE FROM ACCESSORIES. Chevrolet Celebrity 1982

For 1990-2009 cars

# ENGINE ROUGH VOLTAGE SPIKE FROM ACCESSORIES

#### Subject: THROTTLE STOP SCREW PLUG REMOVAL - 1982 VEHICLES EQUIPPED WITH THROTTLE BODY INJECTION

If it becomes necessary to remove the throttle stop screw plug(s) to adjust minimum idle speed on the single TBI 300, or the minimum idle speed and/or throttle balance on the TBI 400 (crossfire injection), the method illustrated permits on-car plug removal. Removal of the unit(s) from the manifold for this purpose is no longer required. Refer to attached illustration.

Refer to figure:

1) FROM TIP, PRICK PUNCH OVER CENTER LINE OF THROTTLE STOP SCREW AS INDICATED

2) DRILL 5/32" DIA. HOLE THRU CASTING TO HARDENED PLUG.

3) USING 1/16" DIA. PUNCH, PUNCH THRU BOTTOM OF DRILLED HOLE TO REMOVE PLUG.

PLEASE NOTE: DO NOT TAMPER WITH THROTTLE STOP SCREW ON THE FRONT INJECTOR OF THE 2 X 1 SYSTEM AS THERE IS CURRENTLY NO PROCEDURE FOR PERFORMING THIS ADJUSTMENT IN THE FIELD.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.