REAR MAIN BEARING CAP GROOVE ELIMINATION. Chevrolet Celebrity 1984

For 1990-2009 cars

# REAR MAIN BEARING CAP GROOVE ELIMINATION

#### Model and Year 1978-80 MONZA, 1980-84 CITATION, AND 1982-84 CELEBRITY AND CAMARO

The groove in the rear main bearing cap, which was used to retain the oil pan gasket seal in prior years, has been eliminated.

This change should have no effect on service procedures other than a reduction in the amount of sealant required for oil pan installation.

Past model service engine blocks, 1982 and prior years, may or may not have the groove and will have to be serviced using the appropriate procedures for the application. Gaskets cannot be used on engines without the bearing cap groove.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.