INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP. Chevrolet Celebrity 1988

For 1990-2009 cars

# INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP

IF AN INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP DUE TO A HEAT DISTORTED SOCKET IS ENCOUNTERED IN A J-37, A-37 OR BUICK REATTA, BOTH SOCKETS MUST BE INSTALLED USING PART NUMBER 5972532 AVAILABLE FROM GMSPO. ALL SERVICE STOCK OF THIS PART USES A NEW HEAT RESISTANT MATERIAL. THE PRODUCTION STOCK WAS CORRECTED BEGINNING WITH THE FOLLOWING VIN BREAKPOINTS:

BUICK JB900864

OLDSMOBILE: JG307649 J9367993 J2336554

PONTIAC: J7544390

CHEVROLET: J7163799 JJ187909

WARRANTY INFORMATION

LABOR OPERATION NUMBER N 1000 LABOR TIME 0.2HRS PART NUMBER 5972532 (2)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1988 OLDSMOBILE DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.