HARSH ENGAGEMENT CONDITIONS SYMPTOMS/DIAGNOSIS/REPAIRS. Chevrolet Celebrity 1988

For 1990-2009 cars

# HARSH ENGAGEMENT CONDITIONS SYMPTOMS/DIAGNOSIS/REPAIRS

#### Model and Year: 1987-88 CELEBRITY WITH THM 440-T4 TRANSAXLE

This bulletin covers harsh engagement conditions and specific service information for 1987-88 Celebrity models equipped with a THM 440-T4 transaxle. Other items which cause harsh engagement conditions are:

- vacuum leaks (low vacuum supply to the vacuum modulator) 33-46 Cm Hg (13-18 In Hg) required - stuck modulator valve - missing #9 checkball

DATE OF PRODUCTION CHANGE: (Figure 1)

November 24, 1987 (Julian Date 328), all THM 440-T4 transaxles were built using a new 1-2 servo cushion spring reverse servo cushion spring and reverse servo return spring.

SERVICE ACTION: (Figure 2)

I. Harsh Engagement From Park Or Neutral To Drive Or Reverse - 1987-88 Without 2.8L Engines

1. Remove the 1-2 servo assembly and the reverse servo assembly from the transaxle. 2. Disassemble and replace the 1-2 servo cushion spring (559) and the reverse servo cushion spring (549) with the correct part listed in the Service Parts Information section. 3. Install the 1-2 servo assembly and reverse servo assembly in the transaxle.

II. Harsh Engagement From Reverse to Drive, Park Or Neutral To Drive Or Reverse - 1987-88 With 2.8 L Engines only

1. Remove the 1-2 servo assembly and the reverse servo assembly from the transaxle. 2. Disassemble and replace the 1-2 servo cushion spring (559), the reverse servo cushion spring (549) and the reverse servo return spring (552) with the parts listed in the Service Parts Information section. 3. Install the 1-2 servo assembly and reverse servo assembly in the transaxle.

SERVICE PARTS INFORMATION:

Part Number Description ---------- ----------- 8668121 Reverse Servo Cushion Spring (549)

8668123 1-2 Servo Cushion Spring (559)

8668127 Reverse Servo Return Spring (552)

SERVICE MANUAL REFERENCE:

Refer to the THM 440-T4 (ME9) Automatic Transaxle On Car Service section for appropriate service information.

#### SERVICE NOTES:

For warranty purposes, use both Labor Operations described below:

Labor Operation K6623 for the reverse servo assembly: 1987-88 - .5 Hour

Labor Operation K6626 for the 1-2 servo assembly: 1987-88 - .5 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.