Technical Service Bulletins Chevrolet Celebrity 1986

For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2008-04-04: 4L60 Automatic Transmission - New Sprag Assembly, Forward Clutch to Overrun Clutch Hub (08-07-30-017)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 1999-12-23: Info - Dealer Installed Rear Seat Lap/Shoulder Belt Kits (99-09-40-006)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1996-03-01: WARRANTY ADMINISTRATION: PANEL REPLACEMENT OPERATIONS (52-05-05)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-10-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51A)
- 1995-09-01: WARRANTY INFORMATION - LABOR TIME SUBMISSION FORMAT (58-05-01A)
- 1995-09-01: REPLACEMENT OF ISOLATION DIODES (93-163-8A)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-19: WARRANTY ADMINISTRATION ADCSM EMPOWERMENT (52-05-06)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-03-01: SMU - SECTION 3D - LOWER MOUNTING BOLT (53-34-01A)
- 1995-02-10: WARRANTY ADMINISTRATION CHEV./GEO ROADSIDE ASSISTANCE (52-05-02)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-02-01: WARRANTY ADMINISTRATION CHEV. CLAIM PROCESSING (42-05-15A)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-11-23: FRONT BRAKE PULSATION - 'NEW' DIAGNOSIS (43-50-09)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-08-16: WARRANTY ADMINISTRATION - CHANGES IN CLAIMS PROCESS (42-05-10)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-20: INFORMATION ON SPEED RATED TIRES (43-35-02)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-04-26: WARRANTY ADMININSTRATION - CLAIM PROCESS CHANGES (42-05-05)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-12-21: SMU - SEC. 3C - FRT. SUSPEN. SPECIFICATION REVISIONS (33-33-03)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-197B-3E)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-227-0B)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-223-7A)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-201-1A)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-04-28: SERVICE MANUAL UPDATE STICKERS (93-183-0A)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-02-01: INDUSTRIAL FALLOUT/RAIL DUST DAMAGE TO BASE COAT/CLEAR COAT (93-58A-10)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (93-6C-100)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-10-16: SCUFF/SCRATCH REMOVAL PROCESS ALUM. WHEEL WITH CLEAR COAT (93-20-3E)
- 1992-10-16: SCUFF/SCRATCH REMOVAL PROCESS ALUM. WHEEL WITH CLEAR COAT (93-10-119)
- 1992-10-01: ENG. MISS, HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (93-35-6D)
- 1992-10-01: INFO EFFECT FUEL VOLATILITY (DRIVEABILITY CONDITIONS) (93-31-6C)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-250-1A)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-232-3E)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-06-02: SLIPS IN LOW/REVERSE NO REVERSE-REPLACE LOW CLUTCH (92-219-7A)
- 1992-06-02: SLIPS IN LOW/REVERSE NO REVERSE-REPLACE LOW CLUTCH (92-73T40-100)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-215-1A)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-147-3E)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-03-20: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (92-130-7A)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-86-7A)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-104)
- 1991-12-20: TIRE COMPANY WARRANTY ASSISTANCE PROGRAM (92-70-3E)
- 1991-12-19: AC-DELCO ADVANCE EXCHANGE PGM. PHONE NUMBER CHANGE (92-97-8C)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-91-7A)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-103)
- 1991-12-14: CHUGGLE AT 56-72 KPH WITH TCC ENGAGED (92-74T60-101)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-42-7A)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-73L80-100)
- 1991-10-11: SELF-ADJUSTER IN REAR CALIPERS NOT FUNCTIONING PROPERLY (88-450-5)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-11-7A)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-74T60-100)
- 1991-08-14: SERVICE GUILD: COOLANT RECYCLING UPDATE (91-0-106)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-05-8A)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-8-102)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-396-7A)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-07-26: AC DELCO ADVANCE EXCHANGE PROGRAMS (REVIEW) (91-388-0A)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-384-6E)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-344-6E)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-6-120)
- 1991-05-15: MULTEC FUEL INJECTORS/CLEANING INFORMATION (91-312-6E)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-334-10)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-2-206)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-22: EXCESS PAINT IN FLYWHEEL MOUNT HOLES (GOODWRENCH MOTOR 2.5L) (86-273-6)
- 1991-04-22: EXCESS PAINT IN FLYWHEEL MOUNT HOLES (GOODWRENCH MOTOR 2.5L) (91-625-105)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-318-6E)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-285-0A)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-2-197)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-251-0B)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-2-175)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (91-2-181)
- 1991-02-20: SERVICE MANUAL UPDATE SEC. 10 UNDER BODY DIMENSION CHANGE (90-405-10)
- 1991-02-20: SERVICE MANUAL UPDATE SEC. 10 UNDER BODY DIMENSION CHANGE (91-2-163)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-213-6D)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-217-6E)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-6-111)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-184-7A)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-73T40-103)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-15: NEW 1-2 AND REVERSE BANDS NO SELECTIVE BAND APPLY PINS (91-120-7A)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-126-8E)
- 1990-12-31: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (90-74T60123)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-31: CHANGE IN BRAKE EFFECTIVENESS AFTER BRAKE WORK (91-133-5)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-140-7A)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-74T60-116)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-142-7A)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-114)
- 1990-10-16: GASKET IN PLACE OF RTV ON ROCKER ARM COVER (91-102-6)
- 1990-10-16: GASKET IN PLACE OF RTV ON ROCKER ARM COVER (91-625-101)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-95-7A)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-108)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-87-7A)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-74T60-109)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-82-7A)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-84-7A)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-85-8A)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (90-73T40110)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-8-108)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-71-7A)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-73T40-100)
- 1990-08-31: (SRTA) MODEL UPDATE W/3T340 (125C) (91-38-7A)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-53-7A)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-74T60-100)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-101)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (91-35-3E)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-293-5)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-118)
- 1990-06-11: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-239-6B)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-7440-117)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-243-7A)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-119)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-219-7A)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (91-10-8A)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-114)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (91-09-0A)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (90-6-107)
- 1990-04-06: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-8-181)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (91-14-8A)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-197-7A)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-112)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-199-6E)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-182-7A)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-111)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-109)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-92-10)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-191-7A)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7440-104)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-277-7A)
- 1989-10-17: LTG REQUEST FOR REVIEW UPDATES JULY THRU OCT. 1989 (90-127-0A)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-7125-116)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-268-0B)
- 1989-09-23: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (89-625-102)
- 1989-09-18: USE GASKET FOR ROCKER ARM COVER INSTEAD OF RTV (90-625-101)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-56-8)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-8-103)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-49-6B)
- 1989-08-18: THM 440-T4/HYDRA-MATIC 4T60 REPAIR GUIDELINES (90-74-7A)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-18: THM 440-T4/HYDRA-MATIC 4T60 REPAIR GUIDELINES (90-7440-101)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-253-1B)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-07-16: LTG REQUEST FOR REVIEW UPDATES 1989 FEB. THRU JUNE 1989 (90-34-0A)
- 1989-06-20: BROKEN CYLINDER HEAD BOLT COOLANT LOSS (NEW BOLT/GASKET) (87-306-6A)
- 1989-06-20: BROKEN CYLINDER HEAD BOLT COOLANT LOSS (NEW BOLT/GASKET) (89-625-111)
- 1989-06-16: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (90-158-6A)
- 1989-06-16: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (90-625-104)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (88-417-3B)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (9S02)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-185-7A)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-109)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (90-17-7A)
- 1989-05-23: TRANSAXLE FINAL DRIVE RATIO -440-T4/4T60 (89-7440-108)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-110)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-171-10)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-2-161)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (90-216-6)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (89-6-115)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (87-304-7A)
- 1989-05-05: REVISE CODE 35/CHT C-2 IAC CHT ALL 82-89 W/IAC SYSTEM (89-177-6E)
- 1989-05-05: REVISE CODE 35/CHT C-2 IAC CHT ALL 82-89 W/IAC SYSTEM (89-6-112)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (89-7-108)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-152-8B)
- 1989-04-19: POWER RACK & PINION GEAR SERVICE INFORMATION (89-153-3B)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-162)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-154-7A)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-7125-109)
- 1989-04-14: GOODWRENCH VEHICLE SECURITY SYSTEM LABOR OPERATIONS (89-146-0A)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-262-5)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-5-116)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-134-7A)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-7440-106)
- 1989-02-28: HESITATION/STALL AFTER COLD START-NEW PROM MAY REPAIR (86-267-6E)
- 1989-02-28: HESITATION/STALL AFTER COLD START-NEW PROM MAY REPAIR (89-628-110)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-127-1B)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-1-112)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-02-01: LABOR TIME GUIDE REQUEST FOR REVIEW CHANGES-sepT/JAN (89-90-0A)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-108-9A)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-8-137)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-96-7A-7B)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-105)
- 1989-01-18: SERVICE GUILD: ON-CAR BRAKE ROTOR TURNING TOOL (89-85-5)
- 1989-01-18: SERVICE GUILD: ON-CAR BRAKE ROTOR TURNING TOOL (89-5-107)
- 1989-01-15: COOLANT FAN SYSTEM DIAGNOSTICS SHOP MANUAL REVISION (86-203)
- 1989-01-15: COOLANT FAN SYSTEM DIAGNOSTICS SHOP MANUAL REVISION (86-8-158)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1989-01-05: HARSH SHIFT CONDITIONS AND CAR SERVICE INFORMATION (89-7440-105)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (89-112-6C)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (88-6-125)
- 1988-12-14: LONGER BRAKE PEDAL TRAVEL DIAGNOSIS AND REPAIR (86-265-5)
- 1988-12-14: LONGER BRAKE PEDAL TRAVEL DIAGNOSIS AND REPAIR (88-5-138)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-31-6C)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6-101)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-38-1B)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-110)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-356-5)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-5-137)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-44-5)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-101)
- 1988-09-20: NEUTRAL/DRIVE TRANSMISSION GEAR RATTLE INFORMATION (88-351-7B)
- 1988-09-20: NEUTRAL/DRIVE TRANSMISSION GEAR RATTLE INFORMATION (88-7-110)
- 1988-09-19: ELECTRIC FUEL PUMP NOISE DIAGNOSIS AND NEW PARTS (88-638-113)
- 1988-09-01: SERVICE GUILD: A/C COMPRESSOR LINES REVERSED DURING SERVICE (88-370-1B)
- 1988-09-01: 1986 FRENCH LABEL INSTALLATION INSTRUCTIONS (86-0-101)
- 1988-09-01: SERVICE GUILD: A/C COMPRESSOR LINES REVERSED DURING SERVICE (88-1-147)
- 1988-08-26: DISC BRAKE NOISE GUIDELINES/DESCRIPTIONS (88-340-5)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-112-7A)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-7440-108)
- 1988-08-26: DISC BRAKE NOISE GUIDELINES/DESCRIPTIONS (88-5-125)
- 1988-08-22: SERVICE GUILD: THE IMPORTANCE OF FOUR WHEEL ALIGNMENT/ALL (89-01-3A)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-08-03: BENCH TYPE SEAT ADJUSTER BINDS REPAIR PROCEDURE (88-321-10)
- 1988-08-03: BENCH TYPE SEAT ADJUSTER BINDS REPAIR PROCEDURE (88-2-214)
- 1988-07-21: BLOWN STOP LIGHT FUSE (NEW WIRE ASSEMBLY P/N) (88-314-8B)
- 1988-07-21: BLOWN STOP LIGHT FUSE (NEW WIRE ASSEMBLY P/N) (88-8-174)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-06-24: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO.TO PREVENT) (88-283-6E)
- 1988-06-24: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO.TO PREVENT) (88-6-118)
- 1988-06-06: SERVICE MANUAL UPDATE UNSTABLE OR INCORRECT IDLE (88-269-6E)
- 1988-06-06: SERVICE MANUAL UPDATE UNSTABLE OR INCORRECT IDLE (88-6-117)
- 1988-05-31: SERVICE MANUAL UPDATE-REVISED CAM GEAR REPLACEMENT PROCEDURE (88-278-6A)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-363-3B)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-3-130)
- 1988-05-31: SERVICE MANUAL UPDATE-REVISED CAM GEAR REPLACEMENT PROCEDURE (88-625-114)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-242-10)
- 1988-05-19: SERVICE GUILD: INSTALLATION OF AFTER MARKET STYLED WHEELS (88-246-3E)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-2-183)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-253-3B)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-128)
- 1988-05-12: ENGINE COOLING SYSTEM LEAKS (DIAGNOSIS INFORMATION) (88-245-6B)
- 1988-05-12: ENGINE COOLING SYSTEM LEAKS (DIAGNOSIS INFORMATION) (88-6-115)
- 1988-05-06: HARD OR NO SHIFT MAY BE LOOSE SHIFT LEVER NUT (88-233-7B)
- 1988-05-06: HARD OR NO SHIFT MAY BE LOOSE SHIFT LEVER NUT (88-7050-110)
- 1988-05-05: NOISY WIRE WHEEL COVERS (PROCEDURE TO DIAGNOSE/REPAIR) (88-225-3E)
- 1988-05-05: NOISY WIRE WHEEL COVERS (PROCEDURE TO DIAGNOSE/REPAIR) (88-2-175)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-207-7A)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-105)
- 1988-04-22: GASOLINE ADDITIVE EXHAUST VALVE RECESSION (86-260-0A)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-209-9A)
- 1988-04-22: GASOLINE ADDITIVE EXHAUST VALVE RECESSION (88-6-112)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-8-149)
- 1988-04-04: THM 440-T4 UPDATE BOOK SUMMARIZES PRODUCT CHANGES (88-7440-105)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-201-7A)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-7440-108)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-171-7A)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-7440-106)
- 1988-02-29: SERVICE MANUAL UPDATE THERMAL ELEMENT ON CAR SERVICE (88-163-7A)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-29: SERVICE MANUAL UPDATE THERMAL ELEMENT ON CAR SERVICE (88-7440-104)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-161-7A)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-7400-101)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-156-7A)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-7125-104)
- 1988-02-15: PROPER SERVICE FLUID FOR MANUAL TRANSAXLE/TRANSMISSION (88-158-7B)
- 1988-02-15: PROPER SERVICE FLUID FOR MANUAL TRANSAXLE/TRANSMISSION (88-7050-106)
- 1988-02-01: ENG. MISS, HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-138-6D)
- 1988-01-25: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-7125-103)
- 1988-01-25: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-8-119)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-125-10)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-2-131)
- 1988-01-13: CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION) (88-130-6A)
- 1988-01-13: CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION) (88-625-103)
- 1988-01-11: REMOVAL OF CHEMICAL SPOTTING AND MINOR PAINT IMPERFECTIONS (88-135-10)
- 1988-01-08: MANUAL SEAT BACK RECLINER COMMENTS (87-262-10)
- 1988-01-08: MANUAL SEAT BACK RECLINER COMMENTS (87-2-252)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-628-123)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-630-108)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-638-113)
- 1988-01-01: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-260-7A)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-142)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-628-111)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-630-103)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-638-108)
- 1987-12-21: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-114-6)
- 1987-12-21: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-628-109)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-118-7A)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-7125-100)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-119-7A)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-7440-102)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-111-7A)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-7440-101)
- 1987-12-03: SERVICE MANUAL UPDATE INFORMATION/ THM 440-T4 (87-261-7A)
- 1987-12-03: SERVICE MANUAL UPDATE INFORMATION/ THM 440-T4 (87-7440-121)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-101-8A)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-117)
- 1987-11-30: VALANCE PANEL WARPED/MISALIGN REPLACEMENT INSTRUCTIONS (87-255-10)
- 1987-11-30: VALANCE PANEL WARPED/MISALIGN REPLACEMENT INSTRUCTIONS (87-2-240)
- 1987-11-16: INOPERATIVE COOLING FAN HIGH A/C HEAD PRESSURE (87-229-1B)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-116-3E)
- 1987-11-16: INOPERATIVE COOLING FAN HIGH A/C HEAD PRESSURE (87-628-120)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (86-258-7A)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (87-7440-105)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-10-09: HARSH 1-2 SHIFT CONDITION CHECK 2ND CLUTCH FEED (87-246-7A)
- 1987-10-09: HARSH 1-2 SHIFT CONDITION CHECK 2ND CLUTCH FEED (87-7440-119)
- 1987-10-07: REAR BRAKE DRUM FREEZE INSTALL NEW BACKING PLATE P/N (87-238-5)
- 1987-10-07: REAR BRAKE DRUM FREEZE INSTALL NEW BACKING PLATE P/N (87-5-117)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-191)
- 1987-10-01: DELAYED SHIFT THM 440-T4 3RD CLUTCH SEAL (87-70)
- 1987-10-01: HIGH IDLE SPEED 86 CELEBRITY (VIN X) ENGINE (86-252-6E)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-104)
- 1987-09-28: GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N (87-234-10)
- 1987-09-28: GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N (87-2-216)
- 1987-09-24: RADIAL TIRE/LEAD PULL CORRECTION CHARTS (87-212-3)
- 1987-09-23: TPS SPECIFICATIONS INFORMATION (88-55)
- 1987-09-23: TPS SPECIFICATIONS INFORMATION (88-628-104)
- 1987-09-15: THM 125C SRTA PROGRAM GUIDELINE INFORMATION (86-251)
- 1987-09-15: RATTLE NOISE FROM TURN SIGNAL LEVER (INSTALL FOAM DONUT) (87-224)
- 1987-09-15: END OF EXCHANGE PROGRAM INFORMATION (88-63-7B)
- 1987-09-15: RATTLE NOISE FROM TURN SIGNAL LEVER (INSTALL FOAM DONUT) (87-2-215)
- 1987-09-08: TRANSMISSION FLEXPLATE CRACKS 2.8 W/ A/T -REPLACE DOWEL PIN (87-219)
- 1987-09-08: TRANSMISSION FLEXPLATE CRACKS 2.8 W/ A/T -REPLACE DOWEL PIN (87-628-119)
- 1987-09-04: ECM RESET/ FAILURE DIAGNOSIS INFORMATION (87-6-117)
- 1987-08-20: STEERING LEAD OR PULL DIAGNOSIS AND POSSIBLE REPAIR (87-3-132)
- 1987-08-18: FUEL PUMP RUN-ON AFTER ENGINE TURNED OFF (87-210)
- 1987-08-14: SERVICE GUILD: SERVICE REPL. ECM WITH PROM INSTALLED (88-42)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-208)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-7440-115)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (86-246)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (87-7440-112)
- 1987-08-03: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-110)
- 1987-08-03: SECOND GEAR STARTS SERVICE ACTION (87-7440-111)
- 1987-07-16: TILT STEERING COLUMN NOISE LUBRICATE LOCK BOLT (87-194)
- 1987-07-16: TILT STEERING COLUMN NOISE LUBRICATE LOCK BOLT (87-3-129)
- 1987-07-07: CAMPAIGN: ANTI-LOCK BRAKE PRESSURE WARNING LIGHT (7A04)
- 1987-07-01: SECOND GEAR STARTS THM-440-T4 TRANSAXLE (87-179)
- 1987-07-01: ANALYSIS OF ENGINES WITH INTERNAL SLUDGE ACCUMULATION (87-182)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-202)
- 1987-06-16: ENGINE FLARE SLIPS NO DRIVE ON TURNS -84-87 THM 440T4 (87-168)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-7440-109)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (87-158)
- 1987-05-29: GASOLINE MARKETED/ADVERTISED KEEP PORT FUEL INJECTORS CLEAN (87-165)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-160)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-7440-117)
- 1987-05-26: COLD START INJECTOR 'O' RING REPLACEMENT (87-153)
- 1987-05-26: COLD START INJECTOR 'O' RING REPLACEMENT (87-628-113)
- 1987-05-14: ENG.MISS, BACKFIRE, HESITATION DELCO 'TYPE II'/ 'DIS' COILS (87-145)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-150)
- 1987-05-14: ENG.MISS, BACKFIRE, HESITATION DELCO 'TYPE II'/ 'DIS' COILS (87-6-112)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-6-115)
- 1987-05-01: HARSH ENGAGEMENT NEUTRAL TO DRIVE OR REVERSE (87-133)
- 1987-05-01: HARSH ENGAGEMENT NEUTRAL TO DRIVE OR REVERSE (87-7125-104)
- 1987-04-30: TIRE /WHEEL VIBRATION EXISTS SPECIAL HANDLING TIRES (87-130)
- 1987-04-30: TIRE /WHEEL VIBRATION EXISTS SPECIAL HANDLING TIRES (87-3-122)
- 1987-04-30: VIBRATION CAUSED BY EXCESSIVE WHEEL RUNOUT (86-3-128)
- 1987-04-21: CS-121 & CS-130 GENERATORS SERVICED BY REPLACEMENT (87-124)
- 1987-04-21: CS-121 & CS-130 GENERATORS SERVICED BY REPLACEMENT (87-6-111)
- 1987-04-10: PARK BRAKE EQUALIZER NOISE INSTALL INSULATOR AS OUTLINED (87-113)
- 1987-04-10: BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND (87-117)
- 1987-04-10: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-111)
- 1987-04-10: BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND (87-5-104)
- 1987-04-10: PARK BRAKE EQUALIZER NOISE INSTALL INSULATOR AS OUTLINED (87-5-107)
- 1987-04-07: ENG. MAY INTERMITTENTLY STALL CHECK FOR RESIDUE ON THROTTLE (87-109)
- 1987-04-07: ENG. MAY INTERMITTENTLY STALL CHECK FOR RESIDUE ON THROTTLE (87-628-109)
- 1987-04-07: METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND ' (87-8-139)
- 1987-04-03: SERVICE REPLACEMENT CRANKSHAFT P/N LISTED (87-101)
- 1987-04-03: SERVICE REPLACEMENT CRANKSHAFT P/N LISTED (87-625-107)
- 1987-04-02: REAR BUMPER BAR CORROSION NEW BAR AND TAIL PIPE P/N'S (87-97)
- 1987-04-02: REAR BUMPER BAR CORROSION NEW BAR AND TAIL PIPE P/N'S (87-2-151)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (89-59-3E)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (87-3-115)
- 1987-03-16: HARD START OR EXTENDED CRANK AFTER HOT OR COLD SOAK (86-227)
- 1987-03-16: HARD START OR EXTENDED CRANK AFTER HOT OR COLD SOAK (86-628-114)
- 1987-02-25: CHARGE INDICATOR LAMP DIAGNOSIS CHECK OUTLINED (87-82)
- 1987-02-25: FUEL STARVATION W/NOSE PARKED DOWN - 1/4 TANK FUEL (87-83)
- 1987-02-25: CHARGE INDICATOR LAMP DIAGNOSIS CHECK OUTLINED (87-6-109)
- 1987-02-25: FUEL STARVATION W/NOSE PARKED DOWN - 1/4 TANK FUEL (87-628-105)
- 1987-02-09: WATER IN COMPOSITE HEADLAMPS CHECK VENT TUBES FOR KINKS (87-77)
- 1987-02-09: REVISED: WATER IN HEADLAMPS CHECK VENT TUBES FOR KINKS (87-2-128)
- 1987-02-09: WATER IN COMPOSITE HEADLAMPS CHECK VENT TUBES FOR KINKS (87-2-130)
- 1987-01-08: TV SYSTEM DIAG.-ALL A/T EXCEPT THM 180,350,400 (87-55)
- 1987-01-08: TV SYSTEM DIAG.-ALL A/T EXCEPT THM 180,350,400 (87-7-101)
- 1987-01-01: MOISTURE/FRONT MARKER LAMPS REPAIR PROCEDURE (86-210R)
- 1987-01-01: MOISTURE/FRONT MARKER LAMPS REPAIR PROCEDURE (86-2-177)
- 1986-12-15: INTERMEDIATE PIPE REPLACEMENT ON ALL WELDED EXHAUST SYSTEMS (86-6-138)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-12-11: ENGINE SURGE MAY NEED SERVICE PROM (86-212)
- 1986-12-11: ENGINE DETONATION/CHUGGLE MAY NEED SERVICE PROM (86-213)
- 1986-12-11: ENGINE SURGE MAY NEED SERVICE PROM (86-628-112)
- 1986-12-11: ENGINE DETONATION/CHUGGLE MAY NEED SERVICE PROM (86-628-113)
- 1986-12-09: LOOSE W/S WIPER ARMS NEW STYLE WIPER ARMS AVAIL. (86-209)
- 1986-12-09: LOOSE W/S WIPER ARMS NEW STYLE WIPER ARMS AVAIL. (86-2-179)
- 1986-12-01: PORT FUEL INJ. REPLACEMENT USAGE AND P/N'S LISTED (87-36)
- 1986-12-01: PORT FUEL INJ. REPLACEMENT USAGE AND P/N'S LISTED (87-628-104)
- 1986-11-12: REDUCE THROTTLE PEDAL EFFORT ELIMINATE RETURN SPRING (87-27)
- 1986-11-12: REDUCE THROTTLE PEDAL EFFORT ELIMINATE RETURN SPRING (87-7440-101)
- 1986-11-07: VIBRATION DIAGNOSIS 'REED' TACHOMETER INFORMATION (87-139)
- 1986-11-07: CLEAN PORT FUEL INJECTORS GASOLINE ADDITIVES (87-25)
- 1986-11-07: CLEAN PORT FUEL INJECTORS GASOLINE ADDITIVES (87-0-106)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-118)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-6-122)
- 1986-10-31: 1986 SHOP MANUAL UPDATE REVISION TO IAC CODE 35 CHART (86-199)
- 1986-10-31: REPETITIVE INOP A/C COMPRESSOR FLUSHING PROCEDURE REVISED (87-21)
- 1986-10-31: 1986 SHOP MANUAL UPDATE REVISION TO IAC CODE 35 CHART (86-625-115)
- 1986-10-31: REPETITIVE INOP A/C COMPRESSOR FLUSHING PROCEDURE REVISED (87-1-102)
- 1986-10-29: HARSH NEUTRAL TO REVERSE/DRIVE CHECK VACUUM LINE FOR BLOCKAGE (87-190)
- 1986-10-29: HARSH NEUTRAL TO REVERSE/DRIVE CHECK VACUUM LINE FOR BLOCKAGE (87-7440-100)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-10-14: NEW TRANSMISSION PAN GASKET- ALL THM 125C (86-7125-101)
- 1986-10-13: HARSH UPSHIFTS/3-2 SHIFTS SERVICE INFORMATION (440-T4) (86-190R)
- 1986-10-13: REVISED: HARSH UPSHIFTS / 3-2 SERVICE INFORMATION (440-T4) (86-170)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-191)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-7440-109)
- 1986-10-06: HARSH UPSHIFTS AT HIGH ALTITUDES (86-7400-108)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (84-102)
- 1986-09-24: REVISED:CHATTERING BLADES CLEAN BLADES/GLASS (84-2-140)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (87-2-106)
- 1986-09-23: COLOR COAT CHIPS OFF GUIDELINES FOR INSPECTION (87-09)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-23: COLOR COAT CHIPS OFF GUIDELINES FOR INSPECTION (87-2-101)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-108)
- 1986-09-15: PAINT/CARE OF CAR FINISHES ALL VEHICLES AFFECTED (87-2-100)
- 1986-09-09: REPLACEMENT PAGE 1986 MANUAL DRIVEABILITY SECTION (86-172)
- 1986-09-09: HARD TO PRESS THROTTLE PEDAL SERVICE KIT FOR E2SE CARB. (86-181R)
- 1986-09-09: REPLACEMENT PAGE 1986 MANUAL DRIVEABILITY SECTION (86-625-112)
- 1986-09-09: HARD TO PRESS THROTTLE PEDAL SERVICE KIT FOR E2SE CARB. (86-628-108)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-169)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-7200-103)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (86-164)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-7-100)
- 1986-09-01: NO UPSHIFT CONDITION AFTER DOWNSHIFT AUTO. TRANSMISSION (86-159)
- 1986-09-01: CAMPAIGN: PUSH-PULL HEADLIGHT SWITCH DEFECTIVE (86-C-05A)
- 1986-08-28: COLOR SANDING NOT RECOMMENDED BASECOAT/CLEARCOAT VEHICLES (86-168)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-07)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-08)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-3-100)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-8-102)
- 1986-08-27: STALL/SURGE AFTER COLD START DIAGNOSIS P/N FOR NEW PROM (86-160)
- 1986-08-27: STALL/SURGE AFTER COLD START DIAGNOSIS P/N FOR NEW PROM (86-628-107)
- 1986-08-26: BLUE EXHAUST TAILPIPE SMOKE REPLACE EXH. VALVE SPRINGS P/N (86-256-6A)
- 1986-08-26: CAMPAIGN:PISTON KNOCK REPLACE PARTIAL ENGINE (86-C-10)
- 1986-08-26: CAMPAIGN:PISTON KNOCK REPLACE PARTIAL ENGINE (6R22)
- 1986-08-26: BLUE EXHAUST TAILPIPE SMOKE REPLACE EXH. VALVE SPRINGS P/N (88-625-102)
- 1986-08-20: REVISION-DIAGNOSTIC ROUTING ON SPECMO C/C QUICK CHECKERS (86-157)
- 1986-08-14: REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY (87-03)
- 1986-08-14: REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY (87-2-103)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-155)
- 1986-08-11: IDLE SPEED SPECS. CORRECTIONS TO SHOP MANUAL (86-625-109)
- 1986-08-11: INOPERATIVE TPS INSTALL HEAT SHIELD (86-625-110)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-7440-104)
- 1986-08-04: REPLACEMENT PAGES 1986 SERVICE MANUALS (86-150)
- 1986-08-04: REPLACEMENT PAGES 1986 SERVICE MANUALS (86-6-125)
- 1986-08-01: HIGH SHIFT EFFORT NON-TILT STEERING WHEEL (86-144)
- 1986-08-01: CAMPAIGN: COLD START VALVE- THERMAL AND TIME SWITCH WIRING (86-C-07)
- 1986-08-01: HIGH SHIFT EFFORT NON-TILT STEERING WHEEL (86-7440-107)
- 1986-07-30: OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C (86-151)
- 1986-07-30: OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C (86-7125-110)
- 1986-07-28: UNLEADED GAS BRANDS PORT FUEL INJECTION (86-147)
- 1986-07-23: DELCO FREEDOM BATTERY DIAGNOSIS-CHARGING INFORMATION (86-187)
- 1986-07-23: DELCO FREEDOM BATTERY DIAGNOSIS-CHARGING INFORMATION (87-8-109)
- 1986-07-21: WIRE WHEEL COVER NOISE INSTALL NYLON CLIPS (85-26)
- 1986-07-21: WIRE WHEEL COVER NOISE INSTALL NYLON CLIPS (84-3-106)
- 1986-07-21: NEW STYLE WIPER ARM VIN BREAK POINTS LISTED (86-2-156)
- 1986-07-21: CEL CODE 52 REVISE DIAG. CHART REVISION TO SHOP MANUAL (86-638-118)
- 1986-07-18: SQUEAK/NOISE DISC BRAKE NEW P/N LINING MATERIAL (86-139)
- 1986-07-18: SQUEAK/NOISE DISC BRAKE NEW P/N LINING MATERIAL (86-5-119)
- 1986-07-17: HIGH EFFORT TO RELASE HOOD LATCH (NEW RELEASE CABLE) (86-135)
- 1986-07-17: HIGH EFFORT TO RELASE HOOD LATCH (NEW RELEASE CABLE) (86-2-161)
- 1986-07-17: IDLE SPEED SPECIFICATIONS CORRECTION TO SHOP MANUAL (86-618-105)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-92)
- 1986-07-15: RACK & PINION POWER STEERING REMANUFACTURED GEARS (86-3-118)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-7-105)
- 1986-07-10: FORWARD CLUTCH HOUSING CHANGE CORRECTS HARSH PARK TO DRIVE (84-267)
- 1986-07-10: FORWARD CLUTCH HOUSING CHANGE CORRECTS HARSH PARK TO DRIVE (86-7125-109)
- 1986-07-03: EXCESSIVE SPARK KNOCK -PING INOPERATIVE EGR VALVE (86-79)
- 1986-07-03: EXCESSIVE SPARK KNOCK -PING INOPERATIVE EGR VALVE (86-625-106)
- 1986-07-02: METHOD OF REMOVING ROCKER ARM COVERS (86-111)
- 1986-07-02: METHOD OF REMOVING ROCKER ARM COVERS (86-625-108)
- 1986-07-01: INOPERATIVE TPS INSTALL HEAT SHIELD (86-122)
- 1986-07-01: V5 A/C COMPRESSOR SERVICEABILITY PART NUMBERS (86-87)
- 1986-07-01: SUPPLEMENT: VARIABLE DISPLACEMENT A/C 'O' RING (86-119)
- 1986-07-01: INOPERATIVE TPS INSTALL HEAT SHIELD (86-618-106)
- 1986-07-01: V5 A/C COMPRESSOR SERVICEABILITY PART NUMBERS (85-1-112)
- 1986-06-20: CLEAR COAT ON ALUMINUM WHEELS REPAIR PROCEDURE OUTLINED (86-131R)
- 1986-06-20: CLEAN, PAINT AND COAT ALL MODELS W/ ALUMINUM WHEELS (84-127)
- 1986-06-20: CLEAN, PAINT & COATING OF ALUMINUM WHEELS (85-3-118)
- 1986-06-16: IRREGULAR/PREMATURE TIRE WEAR REPAIR/ROTATION PROCEDURE (86-90)
- 1986-06-13: AIR CONDITIONING ORIFICE TUBE RELOCATION (86-123)
- 1986-06-13: AIR CONDITIONING ORIFICE TUBE RELOCATION (86-1-106)
- 1986-06-10: REPLACE INTERMEDIATE PIPE WELDED EXHAUST SYSTEMS (86-109)
- 1986-06-10: REPLACE INTERMEDIATE PIPE WELDED EXHAUST SYSTEMS (86-8-134)
- 1986-06-03: HARD TO RELEASE HOOD LATCH CHECK BUMPER AND STRIKER ADJ. (86-103)
- 1986-06-03: HARD TO RELEASE HOOD LATCH CHECK BUMPER AND STRIKER ADJ. (86-2-144)
- 1986-05-30: PREMATURE BRAKE WEAR-BRAKES ENGAGED AFTER PEDAL RELEASED (86-108)
- 1986-05-30: PREMATURE BRAKE WEAR-BRAKES ENGAGED AFTER PEDAL RELEASED (86-5-113)
- 1986-05-30: ANTI-LOCK BRAKE SYSTEM SERVICE MANUAL CORRECTIONS (86-5-116)
- 1986-05-28: ELECTRIC FUEL PUMP HUM NOISE {STATION WAGON} (86-98)
- 1986-05-28: ELECTRIC FUEL PUMP HUM NOISE {STATION WAGON} (86-6-120)
- 1986-05-13: SURGE WHEN TCC ENGAGES NEW PROM P/N TO REVISE TCC (86-100)
- 1986-05-13: SURGE WHEN TCC ENGAGES NEW PROM P/N TO REVISE TCC (86-625-107)
- 1986-05-12: INCORRECT WIRING COLOURS AND TERMINAL ID. ON PG. 6E3-46 (86-0-106)
- 1986-05-12: POWER SUNROOF (OPT CF5) PONTIAC 19&27 BODY STYLES (86-2-137)
- 1986-05-12: SERVICE MANUAL SUPPLEMENT REVISED CARBURETOR NUMBERS (86-6-116)
- 1986-04-28: SCAN TOOL WORKSHOP ALL 1986 VEHICLES (86-6-114)
- 1986-04-23: METRI-PACK 150 TERMINAL TERMINAL REMOVAL INSTRUCTION (86-8-124)
- 1986-04-14: ALUMINUM WHEEL REFINISHING ALL MODELS W/ ALUMINUM WHEELS (86-2-129)
- 1986-04-11: HARSH 1-2 UPSHIFT WHEN HOT 1-2 ACCUM. FEEDBACK ORIFICE (86-91)
- 1986-04-11: HARSH 1-2 UPSHIFT WHEN HOT 1-2 ACCUM. FEEDBACK ORIFICE (86-7125-108)
- 1986-04-10: BUZZ FELT IN ACC. PEDAL NEW SPACER PLATE P/N (86-77)
- 1986-04-10: BUZZ FELT IN ACC. PEDAL NEW SPACER PLATE P/N (86-7125-106)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-83)
- 1986-04-09: BRAKE PULSATIONS DUE TO UNEVEN OR RUSTY ROTOR/BRAKE DRUM (86-84)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-0-108)
- 1986-04-09: BRAKE PULSATIONS DUE TO UNEVEN OR RUSTY ROTOR/BRAKE DRUM (86-5-109)
- 1986-04-04: POPPING NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (85-97)
- 1986-04-04: REVISED:POP NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (86-69)
- 1986-04-04: POPPING NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (86-6-115)
- 1986-03-24: GLOVE BOX DOOR FIT CORRECT ADJUSTMENT (86-67)
- 1986-03-24: METHOD TO REMOVE PUSH ROD COVERS W/O COVER DAMAGE (86-74)
- 1986-03-24: GLOVE BOX DOOR FIT CORRECT ADJUSTMENT (86-2-133)
- 1986-03-24: METHOD TO REMOVE PUSH ROD COVERS W/O COVER DAMAGE (86-625-105)
- 1986-03-20: ROUGH IDLE,SURGE,MISFIRE AND / OR POOR PERFORMANCE (86-64)
- 1986-03-20: ROUGH IDLE,SURGE,MISFIRE AND / OR POOR PERFORMANCE (86-628-101)
- 1986-03-14: ACCESSORY DRIVE BELT TENSION SHOP MANUAL OMISSION (86-63)
- 1986-03-10: POOR COLD DRIVEABILITY HESITATION,STALL,STUMBLE (86-59)
- 1986-03-10: BASECOAT/CLEARCOAT ENAMEL PRODUCTION CHANGE (86-2-120)
- 1986-03-10: INJECTOR FUEL INJECTOR CLEANER TOOL-J35800 (86-6-111)
- 1986-03-04: BASECOAT CLEARCOAT EXTERIOR MACH. POLISH NOT RECOMMENDED (86-45)
- 1986-03-04: BASECOAT CLEARCOAT EXTERIOR MACH. POLISH NOT RECOMMENDED (86-2-126)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-49)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-7-103)
- 1986-02-17: HARSH 1-2 AND 2-3 UP SHIFTS THM 400 (VR-VV) (86-7400-100)
- 1986-02-01: ON-VEHICLE CLEANING OF PORT FUEL INJECTORS (86-19)
- 1986-02-01: NO UPDATE AFTER A PART OR FULL THROTTLE DETENT (85-7-170)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-36)
- 1986-01-31: TRANSAXLE CASE INTERMEDIATE SERVO ORIFICE ELIMINATED (86-40)
- 1986-01-31: SCANNER UPDATE FOR DATA STREAM UPDATE PROCEDURES (86-50)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-6-129)
- 1986-01-31: TRANSAXLE CASE INTERMEDIATE SERVO ORIFICE ELIMINATED (86-7125-105)
- 1986-01-23: THM 125 OR 125C TRANSAXLE SLIPPING IN ALL RANGES (86-32)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-51)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-7-102)
- 1986-01-23: THM 125 OR 125C TRANSAXLE SLIPPING IN ALL RANGES (86-7125-104)
- 1986-01-23: ROUGH IDLE OR POOR PERFORMANCE (CHECK INTAKE PLENUM RUNNERS) (86-34)
- 1986-01-23: ROUGH IDLE OR POOR PERFORMANCE (CHECK INTAKE PLENUM RUNNERS) (86-628-100)
- 1986-01-13: TANDEM DIAPHRAGM POWER BRAKE BOOSTER ASSEMBLY (86-5-105)
- 1986-01-13: INSTRUMENT CLUSTER EXCHANGE -REPAIR PROGRAM (86-8-108)
- 1986-01-02: ENGINE OIL DISCOLORATION OIL LEAK DETECTION (86-25)
- 1985-12-23: WORK AREA & EQUIP. REQUIREMENT TO OVERHAUL TRANSMISSIONS (86-7-101)
- 1985-12-05: VISTA VENT HARDWARE NUT W/INTEGRAL SEAL (85-171)
- 1985-12-05: VISTA VENT HARDWARE NUT W/INTEGRAL SEAL (86-2-113)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-22)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-8-111)
- 1985-12-01: CORRECTION TO DIAGNOSTIC CHARTS SHOP MANUAL (86-14)
- 1985-11-27: IRREGULAR REAR TIRE WEAR TIRE NOISE / ROUGHNESS (86-23)
- 1985-11-27: IRREGULAR REAR TIRE WEAR TIRE NOISE / ROUGHNESS (86-3-107)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-8)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-6-101)
- 1985-11-18: QUIET TURN SIGNAL FLASHERS HIGHER NOISE LEVEL FLASHER P/N (86-6)
- 1985-11-18: BOLT TIGHTENING PROCEDURE CYLINDER HEAD BOLTS (86-625-100)
- 1985-11-18: QUIET TURN SIGNAL FLASHERS HIGHER NOISE LEVEL FLASHER P/N (86-8-110)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-15)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-65)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-2-105)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-7440-101)
- 1985-10-29: RECOMMENDED RTV SEALANTS P/N'S AND APPLICATIONS (86-10)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (85-157)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-100)
- 1985-10-20: POWER BRAKE BOOSTER CHECK VALVE RATTLE-NEW KIT (86-11)
- 1985-10-20: POWER BRAKE BOOSTER CHECK VALVE RATTLE-NEW KIT (86-5-101)
- 1985-10-18: BOLT TIGHTENING PROCEDURE CYLINDER HEAD BOLTS (86-2)
- 1985-10-18: BOLT TIGHTENING PROCEDURE CYLINDER HEAD BOLTS (86-625-103)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (85-146)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (85-9-113)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)
- 1985-10-02: OIL FILTER CHANGE NOT REQUIRED AS A RESULT OF SPARK PLUG FOUL (86-20)
- 1985-10-02: NEW GASKETS: TRANSAXLE OIL PAN AND VALVE BODY COVER (86-76)
- 1985-10-02: NEW TRANSMISSION PAN GASKET ALL THM-125C TRANSMISSIONS (85-130)
- 1985-10-02: REVISED:NEW TRANSAXLE GASKET AND VALVE BODY COVER (86-31)
- 1985-10-02: NEW GASKETS: TRANSAXLE OIL PAN AND VALVE BODY COVER (86-7125-103)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (85-140)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (86-3-101)
- 1985-09-30: TORQUE STEER TO THE RIGHT DIAGNOSIS ASSISTANCE (85-143)
- 1985-09-30: TORQUE STEER TO THE RIGHT DIAGNOSIS ASSISTANCE (86-3-100)
- 1985-09-03: 125 SEAL RING INSTALLATION TOOL AND SIZING TOOL-UPDATE (85-128)
- 1985-09-03: BASECOAT/CLEARCOAT PAINT PLANT PRODUCTION CHANGES (86-86)
- 1985-09-03: BASECOAT/CLEARCOAT PAINT PLANT PRODUCTION CHANGES (86-2-140)
- 1985-09-03: 125 SEAL RING INSTALLATION TOOL AND SIZING TOOL-UPDATE (86-7125-100)
- 1985-09-01: 1986 NEW PRODUCT SERVICE BULLETIN FORMAT (86-0-100)
- 1985-08-13: EXCHANGE PROCEDURE-ELECTRONIC INSTRUMENT CLUSTER (86-0-104)
- 1984-12-17: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (85-6-126)
- 1984-12-01: TANDEM DIAPHRAGM POWER BRAKE BOOSTER SERVICE (86-21)
- 1984-08-13: EMERGENCY PARTS ORDERING PROCEDURE CLARIFICATION (86-48)
- 1984-06-27: TORQUE CONVERTER CLUTCH SHUDDER DIAGNOSIS,125C (84-171)
- 1984-06-27: REVISED:TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (82-T-125)
- 1984-06-27: REVISED:TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (83-T-41)
- 1984-06-27: REVISED: TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (83-T-53)
- 1984-06-27: TORQUE CONVERTER CLUTCH SHUDDER DIAGNOSIS,125C (84-7-147)
- 1984-01-15: REVISED: WIRE WHEEL NOISE INSTALL NYLON CLIPS (84-54)
- 1982-08-09: WINDSHIELD WASHER SPRAY- PATTERN ADJUSTMENT (82-2-128)
- 1982-08-06: MUST AND MILDEW ODOR CAUSE AND CORRECTION (82-I-102)
- 1982-08-06: MUST AND MILDEW ODOR CAUSE AND CORRECTION (82-0-116)